<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<library>
<description>Generated from &lt;b&gt;sd card copier.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="SEEED-CAPACITOR_C0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="SEEED-CAPACITOR_AVX-A">
</package>
<package name="SEEED-CAPACITOR_C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="SEEED-CONNECTOR_H2-2.54">
</package>
<package name="SEEED-CONNECTOR_H2X3-2.54">
</package>
<package name="SEEED-CONNECTOR_MICRO-SD9+4P-SMD-16.1X14.5X1.85MM">
</package>
<package name="SEEED-CONNECTOR_MICRO-USB5+4P-SMD-0.65-B">
</package>
<package name="SEEED-IC_SOT-223">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;</description>
</package>
<package name="SEEED-LED_LED-0603">
</package>
<package name="SEEED-OPL-2017-01-DIODE-JAMES_DO-214AA">
</package>
<package name="SEEED-OPL-2017-01-FUSE-AKITA_F1812">
<description>SMD, 1812(inch)</description>
</package>
<package name="SEEED-OPL-2017-01-IC-AKITA_LQFP64">
<description>LQFP64 (0.5mm pitch)</description>
</package>
<package name="SEEED-OPL-2017-01-IC-AKITA_SOT235">
<description>SOT235</description>
</package>
<package name="SEEED-RESISTOR_R0603">
</package>
<package name="SEEED-SWITCH_SW4-SMD-7.0X3.5X3.5MM-90D">
</package>
<package name="SPARKFUN_OSHW-LOGO-L">
</package>
<package name="SPARKFUN_OSHW-LOGO-M">
</package>
<package name="SPARKFUN_OSHW-LOGO-S">
</package>
<package name="AMINO_CRYSTAL-3.2X2.5">
</package>
<package name="AMINO_SOT143B">
</package>
<package name="CON-LSTB_MA20-2">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="RCL_0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="RCL_0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="RCL_0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="RCL_0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="RCL_0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="RCL_0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="RCL_0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="RCL_0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="RCL_0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="RCL_0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="RCL_0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="RCL_0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="RCL_0411/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 12.5 mm</description>
</package>
<package name="RCL_0411/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 15 mm</description>
</package>
<package name="RCL_0411V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 3.81 mm</description>
</package>
<package name="RCL_0414/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 15 mm</description>
</package>
<package name="RCL_0414V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 5 mm</description>
</package>
<package name="RCL_0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="RCL_0617/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 22.5 mm</description>
</package>
<package name="RCL_0617V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 5 mm</description>
</package>
<package name="RCL_0922/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 22.5 mm</description>
</package>
<package name="RCL_0922V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 7.5 mm</description>
</package>
<package name="RCL_C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="RCL_C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="RCL_C025-030X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 3 x 5 mm</description>
</package>
<package name="RCL_C025-040X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 4 x 5 mm</description>
</package>
<package name="RCL_C025-050X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 5 x 5 mm</description>
</package>
<package name="RCL_C025-060X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 6 x 5 mm</description>
</package>
<package name="RCL_C025_050-024X070">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm + 5 mm, outline 2.4 x 7 mm</description>
</package>
<package name="RCL_C025_050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="RCL_C025_050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="RCL_C025_050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="RCL_C025_050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 + 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="RCL_C050-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="RCL_C050-025X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="RCL_C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="RCL_C050-035X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3.5 x 7.5 mm</description>
</package>
<package name="RCL_C050-045X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 4.5 x 7.5 mm</description>
</package>
<package name="RCL_C050-050X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5 x 7.5 mm</description>
</package>
<package name="RCL_C050-055X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 5.5 x 7.5 mm</description>
</package>
<package name="RCL_C050-075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="RCL_C050H075X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
Horizontal, grid 5 mm, outline 7.5 x 7.5 mm</description>
</package>
<package name="RCL_C075-032X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 3.2 x 10.3 mm</description>
</package>
<package name="RCL_C075-042X103">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 4.2 x 10.3 mm</description>
</package>
<package name="RCL_C075-052X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 5.2 x 10.6 mm</description>
</package>
<package name="RCL_C075-063X106">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 7.5 mm, outline 6.3 x 10.6 mm</description>
</package>
<package name="RCL_C102-043X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 4.3 x 13.3 mm</description>
</package>
<package name="RCL_C102-054X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 5.4 x 13.3 mm</description>
</package>
<package name="RCL_C102-064X133">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm, outline 6.4 x 13.3 mm</description>
</package>
<package name="RCL_C102_152-062X184">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 10.2 mm + 15.2 mm, outline 6.2 x 18.4 mm</description>
</package>
<package name="RCL_C150-054X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 5.4 x 18.3 mm</description>
</package>
<package name="RCL_C150-064X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 6.4 x 18.3 mm</description>
</package>
<package name="RCL_C150-072X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 7.2 x 18.3 mm</description>
</package>
<package name="RCL_C150-084X183">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 8.4 x 18.3 mm</description>
</package>
<package name="RCL_C150-091X182">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 15 mm, outline 9.1 x 18.2 mm</description>
</package>
<package name="RCL_C0201">
<description>Source: http://www.avxcorp.com/docs/catalogs/cx5r.pdf</description>
</package>
<package name="RCL_C225-062X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 6.2 x 26.8 mm</description>
</package>
<package name="RCL_C225-074X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 7.4 x 26.8 mm</description>
</package>
<package name="RCL_C225-087X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 8.7 x 26.8 mm</description>
</package>
<package name="RCL_C225-108X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 10.8 x 26.8 mm</description>
</package>
<package name="RCL_C225-113X268">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.5 mm, outline 11.3 x 26.8 mm</description>
</package>
<package name="RCL_C275-093X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 9.3 x 31.6 mm</description>
</package>
<package name="RCL_C275-113X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 11.3 x 31.6 mm</description>
</package>
<package name="RCL_C275-134X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 13.4 x 31.6 mm</description>
</package>
<package name="RCL_C275-154X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 15.4 x 31.6 mm</description>
</package>
<package name="RCL_C275-173X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 17.3 x 31.6 mm</description>
</package>
<package name="RCL_C275-205X316">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 27.5 mm, outline 20.5 x 31.6 mm</description>
</package>
<package name="RCL_C325-137X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 13.7 x 37.4 mm</description>
</package>
<package name="RCL_C325-162X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 16.2 x 37.4 mm</description>
</package>
<package name="RCL_C325-182X374">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 32.5 mm, outline 18.2 x 37.4 mm</description>
</package>
<package name="RCL_C375-155X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 15.5 x 41.8 mm</description>
</package>
<package name="RCL_C375-192X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 19.2 x 41.8 mm</description>
</package>
<package name="RCL_C375-203X418">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 37.5 mm, outline 20.3 x 41.8 mm</description>
</package>
<package name="RCL_C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C0402K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0204 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1005</description>
</package>
<package name="RCL_C0504">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
<package name="RCL_C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="RCL_C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="RCL_C1005">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="RCL_C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
<package name="RCL_C1310">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C1608">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C1812">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C1812K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1812 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4532</description>
</package>
<package name="RCL_C1825">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C1825K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1825 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 4564</description>
</package>
<package name="RCL_C2012">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C2220K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2220 reflow solder&lt;/b&gt;&lt;p&gt;Metric Code Size 5650</description>
</package>
<package name="RCL_C2225K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 2225 reflow solder&lt;/b&gt;&lt;p&gt;Metric Code Size 5664</description>
</package>
<package name="RCL_C3216">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C3225">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C4532">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_C4564">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RCL_HPC0201">
<description>&lt;b&gt; &lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/10129/hpc0201a.pdf</description>
</package>
<package name="RCL_M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="RCL_M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="RCL_M1406">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="RCL_M2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="RCL_M2309">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="RCL_M3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="RCL_M3516">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="RCL_M5923">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="RCL_MINI_MELF-0102AX">
<description>&lt;b&gt;Mini MELF 0102 Axial&lt;/b&gt;</description>
</package>
<package name="RCL_MINI_MELF-0102R">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0102W">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0204R">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0204W">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0207R">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_MINI_MELF-0207W">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="RCL_P0613/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 15 mm</description>
</package>
<package name="RCL_P0613V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 5 mm</description>
</package>
<package name="RCL_P0817/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 22.5 mm</description>
</package>
<package name="RCL_P0817V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 6.35 mm</description>
</package>
<package name="RCL_R0201">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; chip&lt;p&gt;
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
</package>
<package name="RCL_R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="RCL_R0805W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;</description>
</package>
<package name="RCL_R1005">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R1210W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R1218">
<description>&lt;b&gt;CRCW1218 Thick Film, Rectangular Chip Resistors&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com .. dcrcw.pdf</description>
</package>
<package name="RCL_R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R2010W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R2012W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R2512W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R3216W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R3225">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R3225W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R4527">
<description>&lt;b&gt;Package 4527&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/31059/wsrhigh.pdf</description>
</package>
<package name="RCL_R5025">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="RCL_R5025W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="RCL_R6332">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="RCL_R6332W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="RCL_RDH/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type RDH, grid 15 mm</description>
</package>
<package name="RCL_V234/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V234, grid 12.5 mm</description>
</package>
<package name="RCL_V235/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V235, grid 17.78 mm</description>
</package>
<package name="RCL_V526-0">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V526-0, grid 2.5 mm</description>
</package>
<package name="RCL_VMTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VMTB60">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC60&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA52">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR52&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA53">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR53&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA54">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR54&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_VTA56">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR56&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="RCL_WSC0001">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC01/2">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC0002">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC2515">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC4527">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="RCL_WSC6927">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="TESTPAD_B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_B2,54">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_P1-13Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_P1-17">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_P1-17Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_P1-20">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_P1-20Y">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP06R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP06SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP07R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP07SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP08R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP08SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP09R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP09SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP10R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP10SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP11R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP11SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP12R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP12SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP13R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP13SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP14R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP14SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP15R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP15SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP16R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP16SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP17R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP17SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP18R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP18SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP19R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP19SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
<package name="TESTPAD_TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="SEEED-CAPACITOR_C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SEEED-CAPACITOR_CAP-POLAR">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="SEEED-CONNECTOR_DIP-BLACK-JUMPER">
<pin name="1" function="dotclk"/>
<pin name="2"/>
</symbol>
<symbol name="SEEED-CONNECTOR_HEADER-2X3P">
<pin name="1" function="dotclk"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="SEEED-CONNECTOR_MICRO-SD-CARD-HOLDER-9P">
<pin name="CDN"/>
<pin name="CS"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="G1"/>
<pin name="G2"/>
<pin name="G3"/>
<pin name="G4"/>
<pin name="SCLK"/>
<pin name="VDD"/>
<pin name="VSS"/>
</symbol>
<symbol name="SEEED-CONNECTOR_USB-MICRO-5P">
<pin name="DM"/>
<pin name="DP"/>
<pin name="GND@1"/>
<pin name="GND@2"/>
<pin name="GND@3"/>
<pin name="GND@4"/>
<pin name="GND@5"/>
<pin name="ID"/>
<pin name="VCC"/>
</symbol>
<symbol name="SEEED-IC_PMIC-CJ*1117">
<pin name="GND"/>
<pin name="IN"/>
<pin name="OUT"/>
</symbol>
<symbol name="SEEED-LED_LED-1">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="SEEED-OPL-2017-01-DIODE-JAMES_DIODE*-1">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="SEEED-OPL-2017-01-FUSE-AKITA_FUSE">
<description>general Fuse</description>
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="SEEED-OPL-2017-01-IC-AKITA_24LCXX_5P">
<description>24LCxx, 5p</description>
<pin name="GND" direction="pwr"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD" direction="pwr"/>
<pin name="WP"/>
</symbol>
<symbol name="SEEED-OPL-2017-01-IC-AKITA_STM32F401RET6">
<description>ST Micro, STM32F401RET6</description>
<pin name="BOOT0"/>
<pin name="NRST"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PB10"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC2"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PD2"/>
<pin name="PH0_XI"/>
<pin name="PH1_XO"/>
<pin name="VBAT" direction="pwr"/>
<pin name="VCAP" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD1" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="VDD3" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS1" direction="pwr"/>
<pin name="VSS2" direction="pwr"/>
<pin name="VSS3" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
</symbol>
<symbol name="SEEED-RESISTOR_RES">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SEEED-SWITCH_BUTTON-2+2P">
<pin name="1"/>
<pin name="2"/>
<pin name="S1"/>
<pin name="S2"/>
</symbol>
<symbol name="SPARKFUN_OSHW-LOGO">
</symbol>
<symbol name="SPARKFUN-AESTHETICS_DGND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="AMINO_CRYSTAL">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pas"/>
<pin name="X1" direction="pas"/>
<pin name="X2" direction="pas"/>
</symbol>
<symbol name="AMINO_USB-ESD">
<pin name="GND"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="V+"/>
</symbol>
<symbol name="CON-LSTB_MA20-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
<pin name="19" direction="pas"/>
<pin name="20" direction="pas"/>
<pin name="21" direction="pas"/>
<pin name="22" direction="pas"/>
<pin name="23" direction="pas"/>
<pin name="24" direction="pas"/>
<pin name="25" direction="pas"/>
<pin name="26" direction="pas"/>
<pin name="27" direction="pas"/>
<pin name="28" direction="pas"/>
<pin name="29" direction="pas"/>
<pin name="30" direction="pas"/>
<pin name="31" direction="pas"/>
<pin name="32" direction="pas"/>
<pin name="33" direction="pas"/>
<pin name="34" direction="pas"/>
<pin name="35" direction="pas"/>
<pin name="36" direction="pas"/>
<pin name="37" direction="pas"/>
<pin name="38" direction="pas"/>
<pin name="39" direction="pas"/>
<pin name="40" direction="pas"/>
</symbol>
<symbol name="FRAMES_DOCFIELD">
</symbol>
<symbol name="FRAMES_FRAME_C_L">
</symbol>
<symbol name="RCL_C-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="RCL_R-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SUPPLY1_+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
<symbol name="SUPPLY2_+05V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="TESTPAD_TP">
<pin name="TP" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SEEED-CAPACITOR_CERAMIC-10UF-6.3V-20%-X5R(0402)" prefix="C" uservalue="yes">
<description>302010053</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_C"/>
</gates>
<devices>
<device name="" package="SEEED-CAPACITOR_C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0402MRX5R5BB106"/>
<attribute name="VALUE" value="10uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CAPACITOR_CERAMIC-4.7UF-6.3V-20%-X5R(0402)" prefix="C" uservalue="yes">
<description>302010019</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_C"/>
</gates>
<devices>
<device name="" package="SEEED-CAPACITOR_C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0402MRX5R5BB475"/>
<attribute name="VALUE" value="4.7uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CAPACITOR_CERAMIC-10UF-10V-10%-X5R(0603)" prefix="C" uservalue="yes">
<description>302010103</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_C"/>
</gates>
<devices>
<device name="" package="SEEED-CAPACITOR_C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0603KRX5R6BB106"/>
<attribute name="VALUE" value="10uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CAPACITOR_CERAMIC-100NF-50V-10%-X7R(0603)" prefix="C" uservalue="yes">
<description>302010138</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_C"/>
</gates>
<devices>
<device name="" package="SEEED-CAPACITOR_C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="VALUE" value="100nf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CAPACITOR_TANTALUM-SMD-47UF-6.3V(AVX-A)" prefix="C" uservalue="yes">
<description>302020005</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_CAP-POLAR"/>
</gates>
<devices>
<device name="" package="SEEED-CAPACITOR_AVX-A">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TAJA476*006#NJ"/>
<attribute name="VALUE" value="47uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CONNECTOR_DIP-BLACK-JUMPER" prefix="J" uservalue="yes">
<description>320190003</description>
<gates>
<gate name="G$1" symbol="SEEED-CONNECTOR_DIP-BLACK-JUMPER"/>
</gates>
<devices>
<device name="" package="SEEED-CONNECTOR_H2-2.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CONNECTOR_DIP-BLACK-MALE-HEADER(2X3P-2.54)" prefix="J" uservalue="yes">
<description>320020077</description>
<gates>
<gate name="J" symbol="SEEED-CONNECTOR_HEADER-2X3P"/>
</gates>
<devices>
<device name="-2.54" package="SEEED-CONNECTOR_H2X3-2.54">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="P125-12A1BS116A1"/>
<attribute name="VALUE" value="2x3p-2.54"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CONNECTOR_MICRO-SD-CARD-SOCKET-9P(ST-TF-003A)" prefix="SD">
<description>320090000</description>
<gates>
<gate name="G$1" symbol="SEEED-CONNECTOR_MICRO-SD-CARD-HOLDER-9P"/>
</gates>
<devices>
<device name="" package="SEEED-CONNECTOR_MICRO-SD9+4P-SMD-16.1X14.5X1.85MM">
<connects>
<connect gate="G$1" pin="CDN" pad="9"/>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="DATA1" pad="8"/>
<connect gate="G$1" pin="DATA2" pad="1"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="7"/>
<connect gate="G$1" pin="G1" pad="G1"/>
<connect gate="G$1" pin="G2" pad="G2"/>
<connect gate="G$1" pin="G3" pad="G3"/>
<connect gate="G$1" pin="G4" pad="G4"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ST-TF-003A"/>
<attribute name="VALUE" value="ST-TF-003A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CONNECTOR_MICRO-USB-SMD-B-WITHOUT-POST-W/P(ST-USB-001G)" prefix="USB" uservalue="yes">
<description>320010000</description>
<gates>
<gate name="USB" symbol="SEEED-CONNECTOR_USB-MICRO-5P"/>
</gates>
<devices>
<device name="" package="SEEED-CONNECTOR_MICRO-USB5+4P-SMD-0.65-B">
<connects>
<connect gate="USB" pin="DM" pad="2"/>
<connect gate="USB" pin="DP" pad="3"/>
<connect gate="USB" pin="GND@1" pad="S1"/>
<connect gate="USB" pin="GND@2" pad="S2"/>
<connect gate="USB" pin="GND@3" pad="S3"/>
<connect gate="USB" pin="GND@4" pad="S4 S5 S6"/>
<connect gate="USB" pin="GND@5" pad="5"/>
<connect gate="USB" pin="ID" pad="4"/>
<connect gate="USB" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ST-USB-001G"/>
<attribute name="VALUE" value="ST-USB-001G"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-IC_PMIC-CJT1117-3.3(SOT223)" prefix="U">
<description>310030097</description>
<gates>
<gate name="G$1" symbol="SEEED-IC_PMIC-CJ*1117"/>
</gates>
<devices>
<device name="" package="SEEED-IC_SOT-223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2 TER"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CJT1117-3.3"/>
<attribute name="VALUE" value="CJT1117-3.3-SOT223"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-LED_SMD-LED-CLEAR-BLUE(0603)" prefix="D" uservalue="yes">
<description>304090045</description>
<gates>
<gate name="G$1" symbol="SEEED-LED_LED-1"/>
</gates>
<devices>
<device name="" package="SEEED-LED_LED-0603">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="19-217-BHC-ZL1M2RY-3T"/>
<attribute name="VALUE" value="BLUE-0603"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-LED_SMD-LED-CLEAR-GREEN(0603)" prefix="D" uservalue="yes">
<description>304090043</description>
<gates>
<gate name="G$1" symbol="SEEED-LED_LED-1"/>
</gates>
<devices>
<device name="" package="SEEED-LED_LED-0603">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="19-217-G7C-AN1P2-3T"/>
<attribute name="VALUE" value="GREEN-0603"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-OPL-2017-01-DIODE-JAMES_SMD-DIODE-SCHOTTKY-28V-5A(DO-214AA)" prefix="D" uservalue="yes">
<description>304020021</description>
<gates>
<gate name="G$1" symbol="SEEED-OPL-2017-01-DIODE-JAMES_DIODE*-1"/>
</gates>
<devices>
<device name="" package="SEEED-OPL-2017-01-DIODE-JAMES_DO-214AA">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SS54B"/>
<attribute name="VALUE" value="28V-5A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-OPL-2017-01-FUSE-AKITA_307010004_SMD_PPCT_2000MA_1812" prefix="F">
<description>SMD PPCT-2000mA;1812, 2A-16V, SKU: 307010004</description>
<gates>
<gate name="G$1" symbol="SEEED-OPL-2017-01-FUSE-AKITA_FUSE"/>
</gates>
<devices>
<device name="" package="SEEED-OPL-2017-01-FUSE-AKITA_F1812">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-OPL-2017-01-IC-AKITA_310010495_STM32F401RET6">
<description>ST;STM32F401RET6, SMD IC MCU;LQFP-64, SKU: 310010495</description>
<gates>
<gate name="G$1" symbol="SEEED-OPL-2017-01-IC-AKITA_STM32F401RET6"/>
</gates>
<devices>
<device name="" package="SEEED-OPL-2017-01-IC-AKITA_LQFP64">
<connects>
<connect gate="G$1" pin="BOOT0" pad="P$60"/>
<connect gate="G$1" pin="NRST" pad="P$7"/>
<connect gate="G$1" pin="PA0" pad="P$14"/>
<connect gate="G$1" pin="PA1" pad="P$15"/>
<connect gate="G$1" pin="PA10" pad="P$43"/>
<connect gate="G$1" pin="PA11" pad="P$44"/>
<connect gate="G$1" pin="PA12" pad="P$45"/>
<connect gate="G$1" pin="PA13" pad="P$46"/>
<connect gate="G$1" pin="PA14" pad="P$49"/>
<connect gate="G$1" pin="PA15" pad="P$50"/>
<connect gate="G$1" pin="PA2" pad="P$16"/>
<connect gate="G$1" pin="PA3" pad="P$17"/>
<connect gate="G$1" pin="PA4" pad="P$20"/>
<connect gate="G$1" pin="PA5" pad="P$21"/>
<connect gate="G$1" pin="PA6" pad="P$22"/>
<connect gate="G$1" pin="PA7" pad="P$23"/>
<connect gate="G$1" pin="PA8" pad="P$41"/>
<connect gate="G$1" pin="PA9" pad="P$42"/>
<connect gate="G$1" pin="PB0" pad="P$26"/>
<connect gate="G$1" pin="PB1" pad="P$27"/>
<connect gate="G$1" pin="PB10" pad="P$29"/>
<connect gate="G$1" pin="PB12" pad="P$33"/>
<connect gate="G$1" pin="PB13" pad="P$34"/>
<connect gate="G$1" pin="PB14" pad="P$35"/>
<connect gate="G$1" pin="PB15" pad="P$36"/>
<connect gate="G$1" pin="PB2" pad="P$28"/>
<connect gate="G$1" pin="PB3" pad="P$55"/>
<connect gate="G$1" pin="PB4" pad="P$56"/>
<connect gate="G$1" pin="PB5" pad="P$57"/>
<connect gate="G$1" pin="PB6" pad="P$58"/>
<connect gate="G$1" pin="PB7" pad="P$59"/>
<connect gate="G$1" pin="PB8" pad="P$61"/>
<connect gate="G$1" pin="PB9" pad="P$62"/>
<connect gate="G$1" pin="PC0" pad="P$8"/>
<connect gate="G$1" pin="PC1" pad="P$9"/>
<connect gate="G$1" pin="PC10" pad="P$51"/>
<connect gate="G$1" pin="PC11" pad="P$52"/>
<connect gate="G$1" pin="PC12" pad="P$53"/>
<connect gate="G$1" pin="PC13" pad="P$2"/>
<connect gate="G$1" pin="PC14" pad="P$3"/>
<connect gate="G$1" pin="PC15" pad="P$4"/>
<connect gate="G$1" pin="PC2" pad="P$10"/>
<connect gate="G$1" pin="PC3" pad="P$11"/>
<connect gate="G$1" pin="PC4" pad="P$24"/>
<connect gate="G$1" pin="PC5" pad="P$25"/>
<connect gate="G$1" pin="PC6" pad="P$37"/>
<connect gate="G$1" pin="PC7" pad="P$38"/>
<connect gate="G$1" pin="PC8" pad="P$39"/>
<connect gate="G$1" pin="PC9" pad="P$40"/>
<connect gate="G$1" pin="PD2" pad="P$54"/>
<connect gate="G$1" pin="PH0_XI" pad="P$5"/>
<connect gate="G$1" pin="PH1_XO" pad="P$6"/>
<connect gate="G$1" pin="VBAT" pad="P$1"/>
<connect gate="G$1" pin="VCAP" pad="P$30"/>
<connect gate="G$1" pin="VDD" pad="P$19"/>
<connect gate="G$1" pin="VDD1" pad="P$32"/>
<connect gate="G$1" pin="VDD2" pad="P$48"/>
<connect gate="G$1" pin="VDD3" pad="P$64"/>
<connect gate="G$1" pin="VDDA" pad="P$13"/>
<connect gate="G$1" pin="VSS" pad="P$18"/>
<connect gate="G$1" pin="VSS1" pad="P$31"/>
<connect gate="G$1" pin="VSS2" pad="P$47"/>
<connect gate="G$1" pin="VSS3" pad="P$63"/>
<connect gate="G$1" pin="VSSA" pad="P$12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-OPL-2017-01-IC-AKITA_310090051_24LC32AT-I/OT" prefix="U">
<description>Microchip;24LC32AT-I/OT, SMD IC Memory;SOT-23-5, SKU: 310090051</description>
<gates>
<gate name="G$1" symbol="SEEED-OPL-2017-01-IC-AKITA_24LCXX_5P"/>
</gates>
<devices>
<device name="" package="SEEED-OPL-2017-01-IC-AKITA_SOT235">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SCL" pad="1"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="WP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-RESISTOR_SMD-RES-1M-1%-1/10W(0603)" prefix="R" uservalue="yes">
<description>301010151</description>
<gates>
<gate name="G$1" symbol="SEEED-RESISTOR_RES"/>
</gates>
<devices>
<device name="" package="SEEED-RESISTOR_R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0603FR-071ML"/>
<attribute name="VALUE" value="1M"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-RESISTOR_SMD-RES-3K-1%-1/10W(0603)" prefix="R" uservalue="yes">
<description>301010170</description>
<gates>
<gate name="G$1" symbol="SEEED-RESISTOR_RES"/>
</gates>
<devices>
<device name="" package="SEEED-RESISTOR_R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0603FR-073KL"/>
<attribute name="VALUE" value="3K"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-RESISTOR_SMD-RES-51K-5%-1/10W(0603)" prefix="R" uservalue="yes">
<description>301010145</description>
<gates>
<gate name="G$1" symbol="SEEED-RESISTOR_RES"/>
</gates>
<devices>
<device name="" package="SEEED-RESISTOR_R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0603JR-0751KL"/>
<attribute name="VALUE" value="51K"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-SWITCH_SMD-BUTTON(2+2P-7X3.5MM-90D)" prefix="K" uservalue="yes">
<description>311020023</description>
<gates>
<gate name="K" symbol="SEEED-SWITCH_BUTTON-2+2P"/>
</gates>
<devices>
<device name="" package="SEEED-SWITCH_SW4-SMD-7.0X3.5X3.5MM-90D">
<connects>
<connect gate="K" pin="1" pad="1"/>
<connect gate="K" pin="2" pad="2"/>
<connect gate="K" pin="S1" pad="S1"/>
<connect gate="K" pin="S2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TS-1188E"/>
<attribute name="VALUE" value="TS-1188E"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN_OSHW-LOGO">
<description>&lt;b&gt;Open Source Hardware Logo&lt;/b&gt; This logo indicates the piece of hardware it is found on incorporates a OSHW license and/or adheres to the definition of open source hardware found here: http://freedomdefined.org/OSHW</description>
<gates>
<gate name="G$1" symbol="SPARKFUN_OSHW-LOGO"/>
</gates>
<devices>
<device name="L" package="SPARKFUN_OSHW-LOGO-L">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SPARKFUN_OSHW-LOGO-M">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SPARKFUN_OSHW-LOGO-S">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-AESTHETICS_DGND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-AESTHETICS_DGND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-AESTHETICS_GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="SPARKFUN-AESTHETICS_DGND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMINO_7M-25">
<gates>
<gate name="G$1" symbol="AMINO_CRYSTAL"/>
</gates>
<devices>
<device name="" package="AMINO_CRYSTAL-3.2X2.5">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AMINO_PRTR5V0U2X">
<gates>
<gate name="A" symbol="AMINO_USB-ESD"/>
</gates>
<devices>
<device name="" package="AMINO_SOT143B">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="IO1" pad="2"/>
<connect gate="A" pin="IO2" pad="3"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-LSTB_MA20-2" prefix="SV" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CON-LSTB_MA20-2"/>
</gates>
<devices>
<device name="" package="CON-LSTB_MA20-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="19" pad="19"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="20" pad="20"/>
<connect gate="G$1" pin="21" pad="21"/>
<connect gate="G$1" pin="22" pad="22"/>
<connect gate="G$1" pin="23" pad="23"/>
<connect gate="G$1" pin="24" pad="24"/>
<connect gate="G$1" pin="25" pad="25"/>
<connect gate="G$1" pin="26" pad="26"/>
<connect gate="G$1" pin="27" pad="27"/>
<connect gate="G$1" pin="28" pad="28"/>
<connect gate="G$1" pin="29" pad="29"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="30" pad="30"/>
<connect gate="G$1" pin="31" pad="31"/>
<connect gate="G$1" pin="32" pad="32"/>
<connect gate="G$1" pin="33" pad="33"/>
<connect gate="G$1" pin="34" pad="34"/>
<connect gate="G$1" pin="35" pad="35"/>
<connect gate="G$1" pin="36" pad="36"/>
<connect gate="G$1" pin="37" pad="37"/>
<connect gate="G$1" pin="38" pad="38"/>
<connect gate="G$1" pin="39" pad="39"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="40" pad="40"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAMES_FRAME_C_L" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt; C Size , 17 x 22 INCH, Landscape&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="FRAMES_FRAME_C_L"/>
<gate name="G$2" symbol="FRAMES_DOCFIELD"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RCL_C-EU" prefix="C" uservalue="yes">
<description>&lt;B&gt;CAPACITOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="RCL_C-EU"/>
</gates>
<devices>
<device name="025-024X044" package="RCL_C025-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-025X050" package="RCL_C025-025X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-030X050" package="RCL_C025-030X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-040X050" package="RCL_C025-040X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-050X050" package="RCL_C025-050X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025-060X050" package="RCL_C025-060X050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-025X075" package="RCL_C025_050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-035X075" package="RCL_C025_050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-045X075" package="RCL_C025_050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="025_050-055X075" package="RCL_C025_050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-024X044" package="RCL_C050-024X044">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-025X075" package="RCL_C050-025X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-030X075" package="RCL_C050-030X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-035X075" package="RCL_C050-035X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-045X075" package="RCL_C050-045X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-050X075" package="RCL_C050-050X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-055X075" package="RCL_C050-055X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050-075X075" package="RCL_C050-075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="050H075X075" package="RCL_C050H075X075">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-032X103" package="RCL_C075-032X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-042X103" package="RCL_C075-042X103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-052X106" package="RCL_C075-052X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="075-063X106" package="RCL_C075-063X106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-043X133" package="RCL_C102-043X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-054X133" package="RCL_C102-054X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102-064X133" package="RCL_C102-064X133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="102_152-062X184" package="RCL_C102_152-062X184">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-054X183" package="RCL_C150-054X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-064X183" package="RCL_C150-064X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-072X183" package="RCL_C150-072X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-084X183" package="RCL_C150-084X183">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="150-091X182" package="RCL_C150-091X182">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-062X268" package="RCL_C225-062X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-074X268" package="RCL_C225-074X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-087X268" package="RCL_C225-087X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-108X268" package="RCL_C225-108X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="225-113X268" package="RCL_C225-113X268">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-093X316" package="RCL_C275-093X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-113X316" package="RCL_C275-113X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-134X316" package="RCL_C275-134X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-154X316" package="RCL_C275-154X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-173X316" package="RCL_C275-173X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="275-205X316" package="RCL_C275-205X316">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-137X374" package="RCL_C325-137X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-162X374" package="RCL_C325-162X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="325-182X374" package="RCL_C325-182X374">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-155X418" package="RCL_C375-155X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-192X418" package="RCL_C375-192X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="375-203X418" package="RCL_C375-203X418">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C025_050-024X070" package="RCL_C025_050-024X070">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0201" package="RCL_C0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0402" package="RCL_C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0402K" package="RCL_C0402K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0504" package="RCL_C0504">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603" package="RCL_C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0603K" package="RCL_C0603K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805" package="RCL_C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C0805K" package="RCL_C0805K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1005" package="RCL_C1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206" package="RCL_C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1206K" package="RCL_C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210" package="RCL_C1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1210K" package="RCL_C1210K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1310" package="RCL_C1310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1608" package="RCL_C1608">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812" package="RCL_C1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1812K" package="RCL_C1812K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825" package="RCL_C1825">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C1825K" package="RCL_C1825K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2012" package="RCL_C2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2220K" package="RCL_C2220K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C2225K" package="RCL_C2225K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3216" package="RCL_C3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C3225" package="RCL_C3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4532" package="RCL_C4532">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="C4564" package="RCL_C4564">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HPC0201" package="RCL_HPC0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RCL_R-EU_" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="RCL_R-EU"/>
</gates>
<devices>
<device name="0204/2V" package="RCL_0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/5" package="RCL_0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/7" package="RCL_0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/2V" package="RCL_0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/5V" package="RCL_0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/7" package="RCL_0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/10" package="RCL_0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/12" package="RCL_0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/15" package="RCL_0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/10" package="RCL_0309/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/12" package="RCL_0309/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/V" package="RCL_0309V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/3V" package="RCL_0411V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/12" package="RCL_0411/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/15" package="RCL_0411/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/5V" package="RCL_0414V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/15" package="RCL_0414/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/5V" package="RCL_P0613V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/15" package="RCL_P0613/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/5V" package="RCL_0617V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/17" package="RCL_0617/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/22" package="RCL_0617/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/7V" package="RCL_P0817V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/22" package="RCL_P0817/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922/22" package="RCL_0922/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922V" package="RCL_0922V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M0805" package="RCL_M0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1206" package="RCL_M1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1406" package="RCL_M1406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2012" package="RCL_M2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2309" package="RCL_M2309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3216" package="RCL_M3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3516" package="RCL_M3516">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M5923" package="RCL_M5923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102AX" package="RCL_MINI_MELF-0102AX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102R" package="RCL_MINI_MELF-0102R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102W" package="RCL_MINI_MELF-0102W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204R" package="RCL_MINI_MELF-0204R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204W" package="RCL_MINI_MELF-0204W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207R" package="RCL_MINI_MELF-0207R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207W" package="RCL_MINI_MELF-0207W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0201" package="RCL_R0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0402" package="RCL_R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0603" package="RCL_R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805" package="RCL_R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805W" package="RCL_R0805W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1005" package="RCL_R1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206" package="RCL_R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206W" package="RCL_R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210" package="RCL_R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210W" package="RCL_R1210W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1218" package="RCL_R1218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010" package="RCL_R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010W" package="RCL_R2010W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012" package="RCL_R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012W" package="RCL_R2012W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512" package="RCL_R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512W" package="RCL_R2512W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216" package="RCL_R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216W" package="RCL_R3216W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225" package="RCL_R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225W" package="RCL_R3225W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R4527" package="RCL_R4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025" package="RCL_R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025W" package="RCL_R5025W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332" package="RCL_R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332W" package="RCL_R6332W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RDH/15" package="RCL_RDH/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V234/12" package="RCL_V234/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V235/17" package="RCL_V235/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V526-0" package="RCL_V526-0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VMTA55" package="RCL_VMTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VMTB60" package="RCL_VMTB60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA52" package="RCL_VTA52">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA53" package="RCL_VTA53">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA54" package="RCL_VTA54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA55" package="RCL_VTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA56" package="RCL_VTA56">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC0001" package="RCL_WSC0001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC01/2" package="RCL_WSC01/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC0002" package="RCL_WSC0002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC2515" package="RCL_WSC2515">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC4527" package="RCL_WSC4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC6927" package="RCL_WSC6927">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY1_+3V3" prefix="+3V3">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SUPPLY1_+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SUPPLY2_+5V" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="+5V" symbol="SUPPLY2_+05V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TESTPAD_TP" prefix="TP">
<description>&lt;b&gt;Test pad&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TESTPAD_TP"/>
</gates>
<devices>
<device name="B1,27" package="TESTPAD_B1,27">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="B2,54" package="TESTPAD_B2,54">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-13" package="TESTPAD_P1-13">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-13Y" package="TESTPAD_P1-13Y">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-17" package="TESTPAD_P1-17">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-17Y" package="TESTPAD_P1-17Y">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-20" package="TESTPAD_P1-20">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="PAD1-20Y" package="TESTPAD_P1-20Y">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP06R" package="TESTPAD_TP06R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP06SQ" package="TESTPAD_TP06SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP07R" package="TESTPAD_TP07R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP07SQ" package="TESTPAD_TP07SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP08R" package="TESTPAD_TP08R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP08SQ" package="TESTPAD_TP08SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP09R" package="TESTPAD_TP09R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP09SQ" package="TESTPAD_TP09SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP10R" package="TESTPAD_TP10R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP10SQ" package="TESTPAD_TP10SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP11R" package="TESTPAD_TP11R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP11SQ" package="TESTPAD_TP11SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP12R" package="TESTPAD_TP12R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP12SQ" package="TESTPAD_TP12SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP13R" package="TESTPAD_TP13R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP13SQ" package="TESTPAD_TP13SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP14R" package="TESTPAD_TP14R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP14SQ" package="TESTPAD_TP14SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP15R" package="TESTPAD_TP15R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP15SQ" package="TESTPAD_TP15SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP16R" package="TESTPAD_TP16R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP16SQ" package="TESTPAD_TP16SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP17R" package="TESTPAD_TP17R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP17SQ" package="TESTPAD_TP17SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP18R" package="TESTPAD_TP18R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP18SQ" package="TESTPAD_TP18SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP19R" package="TESTPAD_TP19R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP19SQ" package="TESTPAD_TP19SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP20R" package="TESTPAD_TP20R">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
<device name="TP20SQ" package="TESTPAD_TP20SQ">
<connects>
<connect gate="G$1" pin="TP" pad="TP"/>
</connects>
<technologies>
<technology name="">
<attribute name="TP_SIGNAL_NAME" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
