<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<library>
<description>Generated from &lt;b&gt;growleds.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="GROWLED_4-PLCC">
<description>4-PLCC</description>
</package>
<package name="GROWLED_MOLEX_0475890001">
</package>
<package name="SPARKFUN-AESTHETICS_OSHW-LOGO-L">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Large - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-AESTHETICS_OSHW-LOGO-L_COPPER">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Large - Top Copper&lt;/h3&gt;
&lt;p&gt;Exposed copper logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-AESTHETICS_OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-AESTHETICS_OSHW-LOGO-MINI">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Mini - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-AESTHETICS_OSHW-LOGO-M_COPPER">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Top Copper&lt;/h3&gt;
&lt;p&gt;Exposed copper logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-AESTHETICS_OSHW-LOGO-S">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SPARKFUN-AESTHETICS_OSHW-LOGO-S_COPPER">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Top Copper&lt;/h3&gt;
&lt;p&gt;Exposed copper logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="CON-MOLEX_22-23-2041">
<description>.100" (2.54mm) Center Header - 4 Pin</description>
</package>
</packages>
<symbols>
<symbol name="GROWLED_0475890001">
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND" direction="pwr"/>
<pin name="ID"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="GROWLED_RBLED">
<pin name="PIN1"/>
<pin name="PIN2"/>
<pin name="PIN3"/>
<pin name="PIN4"/>
</symbol>
<symbol name="SPARKFUN-AESTHETICS_OSHW-LOGO">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo&lt;/h3&gt;
&lt;p&gt; This logo indicates the piece of hardware it is found on incorporates a OSHW license and/or adheres to the definition of open source hardware found here: &lt;a href="http://freedomdefined.org/OSHW"&gt;http://freedomdefined.org/OSHW&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Devices using&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</symbol>
<symbol name="CON-MOLEX_M">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="CON-MOLEX_MV">
<pin name="S" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GROWLED_0475890001" prefix="P">
<description>Conn Micro USB Type AB RCP 5 POS 0.65mm Solder RA SMD 5 Terminal 1 Port T/R</description>
<gates>
<gate name="G$1" symbol="GROWLED_0475890001"/>
</gates>
<devices>
<device name="" package="GROWLED_MOLEX_0475890001">
<connects>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value="Conn Micro USB Type AB RCP 5 POS 0.65mm Solder RA SMD 5 Terminal 1 Port T/R"/>
<attribute name="MF" value="Molex"/>
<attribute name="MP" value="0475890001"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="0.46 USD"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GROWLED_RBLED">
<gates>
<gate name="G$1" symbol="GROWLED_RBLED"/>
</gates>
<devices>
<device name="" package="GROWLED_4-PLCC">
<connects>
<connect gate="G$1" pin="PIN1" pad="1"/>
<connect gate="G$1" pin="PIN2" pad="2"/>
<connect gate="G$1" pin="PIN3" pad="3"/>
<connect gate="G$1" pin="PIN4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPARKFUN-AESTHETICS_OSHW-LOGO" prefix="LOGO">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo&lt;/h3&gt;
&lt;p&gt; This logo indicates the piece of hardware it is found on incorporates a OSHW license and/or adheres to the definition of open source hardware found here: &lt;a href="http://freedomdefined.org/OSHW"&gt;http://freedomdefined.org/OSHW&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SPARKFUN-AESTHETICS_OSHW-LOGO"/>
</gates>
<devices>
<device name="L" package="SPARKFUN-AESTHETICS_OSHW-LOGO-L">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L-COPPER" package="SPARKFUN-AESTHETICS_OSHW-LOGO-L_COPPER">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SPARKFUN-AESTHETICS_OSHW-LOGO-M">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M-COPPER" package="SPARKFUN-AESTHETICS_OSHW-LOGO-M_COPPER">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI" package="SPARKFUN-AESTHETICS_OSHW-LOGO-MINI">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SPARKFUN-AESTHETICS_OSHW-LOGO-S">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S-COPPER" package="SPARKFUN-AESTHETICS_OSHW-LOGO-S_COPPER">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CON-MOLEX_22-23-2041" prefix="X">
<description>.100" (2.54mm) Center Header - 4 Pin</description>
<gates>
<gate name="-1" symbol="CON-MOLEX_MV"/>
<gate name="-2" symbol="CON-MOLEX_M"/>
<gate name="-3" symbol="CON-MOLEX_M"/>
<gate name="-4" symbol="CON-MOLEX_M"/>
</gates>
<devices>
<device name="" package="CON-MOLEX_22-23-2041">
<connects>
<connect gate="-1" pin="S" pad="1"/>
<connect gate="-2" pin="S" pad="2"/>
<connect gate="-3" pin="S" pad="3"/>
<connect gate="-4" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2041"/>
<attribute name="OC_FARNELL" value="1462920"/>
<attribute name="OC_NEWARK" value="38C0355"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
