<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<library>
<description>Generated from &lt;b&gt;openautopihat.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="CONNECTOR_2P-1.65-12.1X8.5X13.4H">
</package>
<package name="CONNECTOR_2P-2.54-10.6X10.5X15H">
</package>
<package name="CONNECTOR_2P-3.36">
</package>
<package name="CONNECTOR_2P-5.0">
</package>
<package name="CONNECTOR_4P-3.81-12.7X9X9.3H">
</package>
<package name="CONNECTOR_DB9">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="CONNECTOR_DB9-MEAL">
</package>
<package name="CONNECTOR-_3P-3.5">
</package>
<package name="CONNECTOR-_3P-3.5-10.5X7.4X9.3H">
</package>
<package name="CONNECTOR-_3P-5.08">
</package>
<package name="CONNECTOR-NEW_ANT3-SMD-5.2X3.7X0.7MM">
</package>
<package name="CONNECTOR-NEW_BAT2P-11.55-D12.55-CR1220">
</package>
<package name="CONNECTOR-NEW_BAT2P-13.5-CR1220">
</package>
<package name="CONNECTOR-NEW_BAT2P-20.32-CR2032">
</package>
<package name="CONNECTOR-NEW_BAT2P-SMD-16.4-CR1220">
<description>CR1220 and  CR1225  use this battery holder.</description>
</package>
<package name="CONNECTOR-NEW_BAT2P-SMD-20.5-CR1632">
</package>
<package name="CONNECTOR-NEW_BAT2P-SMD-20.32-CR2032">
</package>
<package name="CONNECTOR-NEW_BAT2P-SMD-23.4-CR2032">
</package>
<package name="DISCRETE_2P-2.0-9.1X3.3">
</package>
<package name="DISCRETE_2P-2.54-9X4.6">
</package>
<package name="DISCRETE_2P-SMD-1.78X1.27">
</package>
<package name="DISCRETE_2P-SMD-3.2X1.5">
</package>
<package name="DISCRETE_2P-SMD-5.08X3.18">
</package>
<package name="DISCRETE_2P-SMD-5X3.2">
<description>3.2mm*5mm dimension &lt;br&gt;
8MHz available</description>
</package>
<package name="DISCRETE_2P-SMD-6X3.6">
<description>3.6mm*6mm dimension &lt;br&gt;
12MHz available</description>
</package>
<package name="DISCRETE_2P-SMD-8X4.5">
<description>4.5mm*8mm dimension &lt;br&gt;
12MHz available</description>
</package>
<package name="DISCRETE_86SMX">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
</package>
<package name="DISCRETE_0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="DISCRETE_0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="DISCRETE_0204SMD">
</package>
<package name="DISCRETE_0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="DISCRETE_0207/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="DISCRETE_0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="DISCRETE_0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="DISCRETE_0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="DISCRETE_0207SMD">
</package>
<package name="DISCRETE_0207V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="DISCRETE_0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="DISCRETE_0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="DISCRETE_0309/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 15mm</description>
</package>
<package name="DISCRETE_0309/20">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 20mm</description>
</package>
<package name="DISCRETE_0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="DISCRETE_0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_0515/20.4">
</package>
<package name="DISCRETE_0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_0821/27">
</package>
<package name="DISCRETE_0824/26">
</package>
<package name="DISCRETE_1206">
</package>
<package name="DISCRETE_1210">
</package>
<package name="DISCRETE_2512">
<description>2512</description>
</package>
<package name="DISCRETE_2512L">
</package>
<package name="DISCRETE_7519-60.4MM">
</package>
<package name="DISCRETE_AVX-A">
</package>
<package name="DISCRETE_AVX-B">
</package>
<package name="DISCRETE_AVX-C">
</package>
<package name="DISCRETE_AVX-D">
</package>
<package name="DISCRETE_AVX-E">
</package>
<package name="DISCRETE_AVX-V">
</package>
<package name="DISCRETE_C0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_C0402S">
</package>
<package name="DISCRETE_C0512/10.18">
<description>FILM CAP 0.01UF/275V</description>
</package>
<package name="DISCRETE_C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_C1206$1">
</package>
<package name="DISCRETE_C1210$1">
</package>
<package name="DISCRETE_CERAMIC-2.54">
</package>
<package name="DISCRETE_CERAMIC-5.08">
</package>
<package name="DISCRETE_CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
<package name="DISCRETE_D1005">
</package>
<package name="DISCRETE_D2010">
<description>&lt;b&gt;1210&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_DO-15">
</package>
<package name="DISCRETE_DO-35">
</package>
<package name="DISCRETE_DO-35-SMD">
</package>
<package name="DISCRETE_DO-41">
</package>
<package name="DISCRETE_DO-41-3.6">
</package>
<package name="DISCRETE_DO-214AB">
<description>SMC&lt;P/&gt;
http://www.vishay.com/docs/88751/88751.pdf</description>
</package>
<package name="DISCRETE_DO-220AA">
<description>http://www.vishay.com/docs/88915/ss1p3l.pdf</description>
</package>
<package name="DISCRETE_ELECTRO-5.3MM">
</package>
<package name="DISCRETE_ELECTRO-8.6MM">
</package>
<package name="DISCRETE_ELECTRO-11.36MM">
</package>
<package name="DISCRETE_ELECTRO-13.5MM">
<description>super capacitance  or  Electrical Doule-Layer Capacitor</description>
</package>
<package name="DISCRETE_ELECTRO-20.5MM">
<description>super capacitance  or  Electrical Doule-Layer Capacitor</description>
</package>
<package name="DISCRETE_ELECTRO-SMD-A-3.8MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package A&lt;/b&gt;</description>
</package>
<package name="DISCRETE_ELECTRO-SMD-B-4.8MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package B&lt;/b&gt;</description>
</package>
<package name="DISCRETE_ELECTRO-SMD-C-6MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package B&lt;/b&gt;</description>
</package>
<package name="DISCRETE_ELECTRO-SMD-D-5.6MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package D&lt;/b&gt;</description>
</package>
<package name="DISCRETE_ELECTRO-SMD-E-7.8MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package E&lt;/b&gt;</description>
</package>
<package name="DISCRETE_ELECTRO-SMD-F-9.6MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package F&lt;/b&gt;</description>
</package>
<package name="DISCRETE_ELECTRO-SMD-G-10MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package G&lt;/b&gt;</description>
</package>
<package name="DISCRETE_ELECTROLYTIC-20.5MM">
</package>
<package name="DISCRETE_HC13U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC18U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC18U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC33U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC33U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC49GW">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC49TL-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC49U-H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC49U-LM">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC49U70">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_LED-2P-2.54-3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="DISCRETE_LED-2P-2.54-4.8X2.54">
</package>
<package name="DISCRETE_LED-2P-2.54-5MM">
</package>
<package name="DISCRETE_LED-2P-2.54-6MM">
</package>
<package name="DISCRETE_LED-2P-2.54-6MM-45D">
</package>
<package name="DISCRETE_LED-2P-2.54-8.5X5-90D">
</package>
<package name="DISCRETE_LED-0603">
</package>
<package name="DISCRETE_LED-0805">
</package>
<package name="DISCRETE_MM20SS">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_MM39SL">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_SM49">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_SMA">
</package>
<package name="DISCRETE_SMB">
</package>
<package name="DISCRETE_SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
<package name="DISCRETE_SOD123-2.7X1.6">
</package>
<package name="DISCRETE_SOD323">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_SOD523">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_TC26V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE_TC38H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_AVX-A">
</package>
<package name="DISCRETE-NEW_AVX-B">
</package>
<package name="DISCRETE-NEW_AVX-C">
</package>
<package name="DISCRETE-NEW_AVX-D">
</package>
<package name="DISCRETE-NEW_AVX-E">
</package>
<package name="DISCRETE-NEW_AVX-V">
</package>
<package name="DISCRETE-NEW_C0201">
</package>
<package name="DISCRETE-NEW_C0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE-NEW_C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE-NEW_C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE-NEW_C1206">
</package>
<package name="DISCRETE-NEW_C1210">
</package>
<package name="DISCRETE-NEW_ELECTRO-SMD-A-3.8MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package A&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_ELECTRO-SMD-B-4.8MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package B&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_ELECTRO-SMD-C-6MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package B&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_ELECTRO-SMD-D-5.6MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package D&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_ELECTRO-SMD-E-7.8MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package E&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_ELECTRO-SMD-F-9.6MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package F&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_ELECTRO-SMD-G-10MM">
<description>&lt;b&gt;Aluminium Electrolytic Capacitor Package G&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_HC49US">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_INT2-3.5-D6.5XH8.0MM">
</package>
<package name="DISCRETE-NEW_INT2-SMD-4.8X4.6X1.0MM">
</package>
<package name="DISCRETE-NEW_INT2-SMD-4.8X4.8X3MM">
</package>
<package name="DISCRETE-NEW_L0201">
</package>
<package name="DISCRETE-NEW_L0402">
</package>
<package name="DISCRETE-NEW_L0420">
</package>
<package name="DISCRETE-NEW_L0603">
</package>
<package name="DISCRETE-NEW_L0630">
<description>06 for width 6.0mm ,30 for height 3.0mm</description>
</package>
<package name="DISCRETE-NEW_L0805">
</package>
<package name="DISCRETE-NEW_L0806">
<description>&lt;b&gt;datasheet:&lt;br&gt;
&lt;u&gt;http://search.murata.co.jp/Ceramy/image/img/PDF/ENG/L0075S0103LQH2MC_02.pdf</description>
</package>
<package name="DISCRETE-NEW_L1616">
</package>
<package name="DISCRETE-NEW_L1813">
<description>&lt;b&gt;1813&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE-NEW_L2020">
</package>
<package name="DISCRETE-NEW_L2218">
<description>http://www.vishay.com/docs/34096/idcp2218.pdf</description>
</package>
<package name="DISCRETE-NEW_L2626">
<description>Low Profile ,High Current IHLP Inductor 6.47mm*6.47*2.4mm</description>
</package>
<package name="DISCRETE-NEW_L5020">
</package>
<package name="DISCRETE-NEW_L5040S">
</package>
<package name="DISCRETE-NEW_PC-D2.286XL5.08MM">
</package>
<package name="DISCRETE-NEW_PC-D5.3MM">
</package>
<package name="DISCRETE-NEW_PC-D8.2MM">
</package>
<package name="DISCRETE-NEW_PC-D8.6MM">
</package>
<package name="DISCRETE-NEW_PC-D11.36MM">
</package>
<package name="DISCRETE-NEW_PC-D13.5MM">
<description>super capacitance  or  Electrical Doule-Layer Capacitor</description>
</package>
<package name="DISCRETE-NEW_PC-D20.5MM">
</package>
<package name="DISCRETE-NEW_PIO73">
</package>
<package name="DISCRETE-NEW_PIO105">
</package>
<package name="DISCRETE-NEW_R0201">
</package>
<package name="DISCRETE-NEW_R0204_5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="DISCRETE-NEW_R0204_7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="DISCRETE-NEW_R0207_7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="DISCRETE-NEW_R0207_10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="DISCRETE-NEW_R0207_12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="DISCRETE-NEW_R0309_10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="DISCRETE-NEW_R0309_12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="DISCRETE-NEW_R0309_15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 15mm</description>
</package>
<package name="DISCRETE-NEW_R0309_20">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 20mm</description>
</package>
<package name="DISCRETE-NEW_R0402">
</package>
<package name="DISCRETE-NEW_R0515_20.4">
</package>
<package name="DISCRETE-NEW_R0603">
</package>
<package name="DISCRETE-NEW_R0805">
</package>
<package name="DISCRETE-NEW_R0821_27">
</package>
<package name="DISCRETE-NEW_R0824_26">
</package>
<package name="DISCRETE-NEW_R1206">
</package>
<package name="DISCRETE-NEW_R2512">
<description>2512</description>
</package>
<package name="DISCRETE-NEW_R7519_60.4">
</package>
<package name="DISCRETE-NEW_SOT-23">
<description>&lt;b&gt;SOT23&lt;/b&gt;</description>
</package>
<package name="DISCRETE-NEW_TP-80X40MIL">
</package>
<package name="DISCRETE-NEW_TP-D23MIL">
</package>
<package name="DISCRETE-NEW_TP-D45MIL">
</package>
<package name="DISCRETE-NEW_TP-D65/35MIL">
</package>
<package name="DISCRETE-NEW_TP-D86MIL">
</package>
<package name="DISCRETE-NEW_TP-D100MIL">
</package>
<package name="DISCRETE-NEW_X2-2.0-D9.1XL3.3MM">
</package>
<package name="DISCRETE-NEW_X2-SMD-2.5X2.0X0.5MM">
</package>
<package name="DISCRETE-NEW_X2-SMD-3.2X1.5X0.55MM">
</package>
<package name="DISCRETE-NEW_X2-SMD-5.0X3.2X1.3MM">
<description>3.2mm*5mm dimension &lt;br&gt;
8MHz available</description>
</package>
<package name="DISCRETE-NEW_X2-SMD-L2.0X1.2X0.55MM">
</package>
<package name="DISCRETE-NEW_X4-SMD-3.2X2.5X0.7MM">
</package>
<package name="DISCRETE-NEW_X4-SMD-6.9X1.4X1.3MM">
</package>
<package name="FOR_TEST_ALBERT_DC-404">
</package>
<package name="IC_SOIC8-6.0">
</package>
<package name="IC_SOIC18">
</package>
<package name="IC-NEW_DFN6-0.5-1.5X1.2X0.72MM">
</package>
<package name="IC-NEW_HWSON8-0.5-2X3X0.75MM">
</package>
<package name="IC-NEW_SOT-89">
<description>SOT98 Emitter Collector Basis</description>
</package>
<package name="IC-NEW_SOT-223">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;</description>
</package>
<package name="IC-NEW_TO-220">
</package>
<package name="IC-NEW_TO-252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="SEEED-CAPACITOR_C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="SEEED-CAPACITOR_C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="SEEED-CONNECTOR_H6-2.54">
</package>
<package name="SEEED-IC_TSSOP20-0.65-6.5X4.4MM">
</package>
<package name="SEEED-INDUCTOR_L0402">
</package>
<package name="SEEED-RESISTOR_R0603">
</package>
<package name="SEEED-RESISTOR_R0805">
</package>
<package name="DISCRETE_1P-D6MM">
</package>
<package name="DISCRETE_2P-6*8H">
</package>
<package name="DISCRETE_2P-ROUND-11.4MM">
</package>
<package name="DISCRETE_2P-SMD-D8.0MM">
</package>
<package name="DISCRETE_5P-19.0X15.5X15.8H">
</package>
<package name="DISCRETE_0806">
<description>&lt;b&gt;datasheet:&lt;br&gt;
&lt;u&gt;http://search.murata.co.jp/Ceramy/image/img/PDF/ENG/L0075S0103LQH2MC_02.pdf</description>
</package>
<package name="DISCRETE_1616BZ">
</package>
<package name="DISCRETE_1813">
<description>&lt;b&gt;1813&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="DISCRETE_2020BZ">
</package>
<package name="DISCRETE_2218">
<description>http://www.vishay.com/docs/34096/idcp2218.pdf</description>
</package>
<package name="DISCRETE_2626">
<description>Low Profile ,High Current IHLP Inductor 6.47mm*6.47*2.4mm</description>
</package>
<package name="DISCRETE_5020">
</package>
<package name="DISCRETE_DO-214AC">
<description>http://www.sycelectronica.com.ar/semiconductores/1N4007-SMD.pdf</description>
</package>
<package name="DISCRETE_L0402">
</package>
<package name="DISCRETE_L0402S">
</package>
<package name="DISCRETE_L0420">
<description>04 for width 4.0mm ,20 for height 2.0mm</description>
</package>
<package name="DISCRETE_L0603">
</package>
<package name="DISCRETE_L0603S">
</package>
<package name="DISCRETE_L0630">
<description>06 for width 6.0mm ,30 for height 3.0mm</description>
</package>
<package name="DISCRETE_L0805">
</package>
<package name="DISCRETE_LED-0402">
</package>
<package name="DISCRETE_LED-1206">
</package>
<package name="DISCRETE_LED-3528">
</package>
<package name="DISCRETE_LED-SIDE-VIEW-0603-LEFT">
</package>
<package name="DISCRETE_LED-SIDE-VIEW-0603-RIGHT">
</package>
<package name="DISCRETE_LL-34">
</package>
<package name="DISCRETE_NPN1.27">
</package>
<package name="DISCRETE_PAD_4080">
</package>
<package name="DISCRETE_PIO73">
</package>
<package name="DISCRETE_PIO105">
</package>
<package name="DISCRETE_R0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="DISCRETE_R0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="DISCRETE_R0204SMD">
</package>
<package name="DISCRETE_R0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="DISCRETE_R0207/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="DISCRETE_R0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="DISCRETE_R0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="DISCRETE_R0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="DISCRETE_R0207SMD">
</package>
<package name="DISCRETE_R0207V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="DISCRETE_R0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="DISCRETE_R0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="DISCRETE_R0309/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 15mm</description>
</package>
<package name="DISCRETE_R0309/20">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 20mm</description>
</package>
<package name="DISCRETE_R0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="DISCRETE_R0402">
</package>
<package name="DISCRETE_R0402S">
</package>
<package name="DISCRETE_R0515/20.4">
</package>
<package name="DISCRETE_R0603">
</package>
<package name="DISCRETE_R0805">
</package>
<package name="DISCRETE_R0821/27">
</package>
<package name="DISCRETE_R0824/26">
</package>
<package name="DISCRETE_R1206">
</package>
<package name="DISCRETE_R2512">
<description>2512</description>
</package>
<package name="DISCRETE_R7519/60.4">
</package>
<package name="DISCRETE_SOT23">
<description>&lt;b&gt;SOT23&lt;/b&gt;</description>
</package>
<package name="DISCRETE_SOT323">
<description>SC-70:3-lead</description>
</package>
<package name="DISCRETE_TO-92-TRIANGLE">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="DISCRETE_TP_3535">
</package>
<package name="DISCRETE_TP_4545">
</package>
<package name="MOUDLE-NEW_LGA18-1.1-9.7X10.1X2.5MM">
</package>
<package name="RASPBERRYPI_BASTELSTUBE_V13_RASPI_GPIO_AB_BOX">
<description>26-pin box header for Raspberry Pi GPIO&lt;br/&gt;
 &amp;nbsp; for use with flat ribbon cables</description>
</package>
<package name="RASPBERRYPI_BASTELSTUBE_V13_RASPI_GPIO_AB_PIN">
<description>26-pin connector for Raspberry Pi GPIO&lt;br/&gt;
 &amp;nbsp; just the two rows of pins</description>
</package>
<package name="TEMPLATE_TSOT23-8">
</package>
</packages>
<symbols>
<symbol name="CONNECTOR_DB9">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="10"/>
<pin name="11"/>
</symbol>
<symbol name="CONNECTOR_SCREW-TERMINAL-2P">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="CONNECTOR-_TER_3.5X3">
<pin name="P$1" function="dotclk"/>
<pin name="P$2"/>
<pin name="P$3"/>
</symbol>
<symbol name="CONNECTOR-NEW_ANTENNA-U-FL">
<pin name="D" function="dotclk"/>
<pin name="GND1"/>
<pin name="GND2"/>
</symbol>
<symbol name="CONNECTOR-NEW_BAT-HOLDER">
<pin name="V+"/>
<pin name="V-"/>
</symbol>
<symbol name="DISCRETE_C@1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DISCRETE_CAPACITOR">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="DISCRETE_DIODE">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="DISCRETE_JP_SW-1">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="DISCRETE_LED">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="DISCRETE_Q">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DISCRETE_R">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DISCRETE-NEW_C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DISCRETE-NEW_CAP-POLAR">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="DISCRETE-NEW_CRYSTAL">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DISCRETE-NEW_DIODE-BAT54C">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
</symbol>
<symbol name="DISCRETE-NEW_L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DISCRETE-NEW_RES-ARRAY">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DISCRETE-NEW_TEST-POINT">
<pin name="T"/>
</symbol>
<symbol name="FOR_TEST_ALBERT_DC-404">
<pin name="+"/>
<pin name="-"/>
<pin name="CDN"/>
</symbol>
<symbol name="IC_MCP2515">
<pin name="!CS" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="!RX0BF" direction="out"/>
<pin name="!RX1BF" direction="out"/>
<pin name="!TX0RTS" direction="in"/>
<pin name="!TX1RTS" direction="in"/>
<pin name="!TX2RTS" direction="in"/>
<pin name="CLKOUT/SOF" direction="out"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="RXCAN" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="TXCAN" direction="out"/>
<pin name="VDD" direction="sup"/>
<pin name="VSS" direction="sup"/>
</symbol>
<symbol name="IC_MCP2551">
<pin name="CANH"/>
<pin name="CANL"/>
<pin name="RS"/>
<pin name="RXD"/>
<pin name="TXD"/>
<pin name="VDD"/>
<pin name="VREF"/>
<pin name="VSS"/>
</symbol>
<symbol name="IC-NEW_AMPLIFIER-MAX2659">
<pin name="!SHDN"/>
<pin name="GND" direction="sup"/>
<pin name="GND@1" direction="sup"/>
<pin name="RFIN"/>
<pin name="RFOUT"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="IC-NEW_PMIC-CJ*1117">
<pin name="GND"/>
<pin name="IN"/>
<pin name="OUT"/>
</symbol>
<symbol name="IC-NEW_RTC-PCF85063TP">
<pin name="!INT"/>
<pin name="CLKOUT"/>
<pin name="OSCI"/>
<pin name="OSCO"/>
<pin name="PAD"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="VDD"/>
<pin name="VSS"/>
</symbol>
<symbol name="POWER-OR-GND-_GND_POWER">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="SEEED-CAPACITOR_C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SEEED-CONNECTOR_HEADER-6P">
<pin name="1" function="dotclk"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
</symbol>
<symbol name="SEEED-IC_TRANSLATOR-TXS0108E">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="GND"/>
<pin name="OE"/>
<pin name="VCCA"/>
<pin name="VCCB"/>
</symbol>
<symbol name="SEEED-INDUCTOR_SMD-INDUCTOR-4.7NH-0.3NH-300MA(0402)">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SEEED-RESISTOR_RES">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DISCRETE_L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DISCRETE_NPN">
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
</symbol>
<symbol name="DISCRETE_RELAY">
<pin name="COM"/>
<pin name="NC"/>
<pin name="NO"/>
<pin name="V+"/>
<pin name="V-"/>
</symbol>
<symbol name="DISCRETE_TEST_POINT">
<pin name="T"/>
</symbol>
<symbol name="MOUDLE-NEW_MOUDLE-GPS-L70-HARDWARE">
<pin name="1PPS"/>
<pin name="ANTON"/>
<pin name="GND" direction="sup"/>
<pin name="GND@1" direction="sup"/>
<pin name="GND@2"/>
<pin name="NC"/>
<pin name="NC@1"/>
<pin name="RESERVED"/>
<pin name="RESERVED1"/>
<pin name="RESET"/>
<pin name="RF_IN"/>
<pin name="RXD1"/>
<pin name="STANDBY"/>
<pin name="TIMER"/>
<pin name="TXD1"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC_RF" direction="pwr"/>
<pin name="V_BCKP"/>
</symbol>
<symbol name="RASPBERRYPI_BASTELSTUBE_V13_RASPI_GPIO_AB">
<description>Generic schematic symbol for the Raspberry Pi GPIO connector&lt;br/&gt;
Model A / B, Revision 2 &amp;nbsp; with 6 &amp;quot;not connected&amp;quot; pins</description>
<pin name="3V3" direction="pwr"/>
<pin name="5V0" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO04"/>
<pin name="GPIO17"/>
<pin name="GPIO18"/>
<pin name="GPIO22"/>
<pin name="GPIO23"/>
<pin name="GPIO24"/>
<pin name="GPIO25"/>
<pin name="GPIO27"/>
<pin name="N.C.0" direction="nc"/>
<pin name="N.C.1" direction="nc"/>
<pin name="N.C.2" direction="nc"/>
<pin name="N.C.3" direction="nc"/>
<pin name="N.C.4" direction="nc"/>
<pin name="N.C.5" direction="nc"/>
<pin name="RXD"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="SPI_CE0"/>
<pin name="SPI_CE1"/>
<pin name="SPI_MISO"/>
<pin name="SPI_MOSI"/>
<pin name="SPI_SCLK"/>
<pin name="TXD"/>
</symbol>
<symbol name="TEMPLATE_MP1496">
<pin name="BS"/>
<pin name="EN/SYNC"/>
<pin name="FB"/>
<pin name="GND"/>
<pin name="IN"/>
<pin name="SS"/>
<pin name="SW"/>
<pin name="VCC"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CONNECTOR_DB9" prefix="J" uservalue="yes">
<gates>
<gate name="G$1" symbol="CONNECTOR_DB9"/>
</gates>
<devices>
<device name="FEMAL" package="CONNECTOR_DB9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="G1"/>
<connect gate="G$1" pin="11" pad="G2"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MEAL" package="CONNECTOR_DB9-MEAL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="G1"/>
<connect gate="G$1" pin="11" pad="G2"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONNECTOR_SCREW-TERMINAL-2P" prefix="J" uservalue="yes">
<gates>
<gate name="G$1" symbol="CONNECTOR_SCREW-TERMINAL-2P"/>
</gates>
<devices>
<device name="1.65" package="CONNECTOR_2P-1.65-12.1X8.5X13.4H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2.54" package="CONNECTOR_2P-2.54-10.6X10.5X15H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.36" package="CONNECTOR_2P-3.36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.81" package="CONNECTOR_4P-3.81-12.7X9X9.3H">
<connects>
<connect gate="G$1" pin="1" pad="1 2"/>
<connect gate="G$1" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.0" package="CONNECTOR_2P-5.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONNECTOR-_SCREW-TERMINAL-3P" prefix="J" uservalue="yes">
<gates>
<gate name="G$1" symbol="CONNECTOR-_TER_3.5X3"/>
</gates>
<devices>
<device name="" package="CONNECTOR-_3P-3.5-10.5X7.4X9.3H">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5" package="CONNECTOR-_3P-3.5">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.08" package="CONNECTOR-_3P-5.08">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONNECTOR-NEW_ANTENNA-ACD5036" prefix="ANT" uservalue="yes">
<gates>
<gate name="G$1" symbol="CONNECTOR-NEW_ANTENNA-U-FL"/>
</gates>
<devices>
<device name="" package="CONNECTOR-NEW_ANT3-SMD-5.2X3.7X0.7MM">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="ACD-5036-A3-CC-S"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CONNECTOR-NEW_BAT-HOLDER" prefix="BAT" uservalue="yes">
<description>BAT2P-13.5-CR1220:320170002;BAT2P-SMD-20.5-CR1632:320170007;METAL-CR2032-D20.0*H6.3MM:320170003;METAL-CR2032-SMD:320170006;PLASTIC-CR1220-L15.06*W13.0*H4.1MM:320170000;PLASTIC-CR2032-L25.2*W15.6*H5.2MM:320170005;BAT2P-11.55-D12.55-CR1220:313010022</description>
<gates>
<gate name="G$1" symbol="CONNECTOR-NEW_BAT-HOLDER"/>
</gates>
<devices>
<device name="12.5" package="CONNECTOR-NEW_BAT2P-11.55-D12.55-CR1220">
<connects>
<connect gate="G$1" pin="V+" pad="+"/>
<connect gate="G$1" pin="V-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2032-SMD" package="CONNECTOR-NEW_BAT2P-SMD-23.4-CR2032">
<connects>
<connect gate="G$1" pin="V+" pad="+"/>
<connect gate="G$1" pin="V-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CR1632" package="CONNECTOR-NEW_BAT2P-SMD-20.5-CR1632">
<connects>
<connect gate="G$1" pin="V+" pad="1 2"/>
<connect gate="G$1" pin="V-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-1220" package="CONNECTOR-NEW_BAT2P-SMD-16.4-CR1220">
<connects>
<connect gate="G$1" pin="V+" pad="+"/>
<connect gate="G$1" pin="V-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1220" package="CONNECTOR-NEW_BAT2P-13.5-CR1220">
<connects>
<connect gate="G$1" pin="V+" pad="+1 +2"/>
<connect gate="G$1" pin="V-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2032" package="CONNECTOR-NEW_BAT2P-20.32-CR2032">
<connects>
<connect gate="G$1" pin="V+" pad="2 3"/>
<connect gate="G$1" pin="V-" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D20.32" package="CONNECTOR-NEW_BAT2P-SMD-20.32-CR2032">
<connects>
<connect gate="G$1" pin="V+" pad="V1 V2"/>
<connect gate="G$1" pin="V-" pad="V-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_C*" prefix="C" uservalue="yes">
<description>&lt;b&gt;Ceramic Capacitors&lt;b&gt;</description>
<gates>
<gate name="C" symbol="DISCRETE_C@1"/>
</gates>
<devices>
<device name="-0402S" package="DISCRETE_C0402S">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2.54" package="DISCRETE_CERAMIC-2.54">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.08" package="DISCRETE_CERAMIC-5.08">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="DISCRETE_C0402">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0512" package="DISCRETE_C0512/10.18">
<connects>
<connect gate="C" pin="1" pad="P$1"/>
<connect gate="C" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="DISCRETE_C0603">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0805" package="DISCRETE_C0805">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1206" package="DISCRETE_C1206$1">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1210" package="DISCRETE_C1210$1">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_CAP*" prefix="C" uservalue="yes">
<description>&lt;b&gt;Electrolytic Capacitors,Tantalum Capacitors and Super Capacitors&lt;/b&gt;</description>
<gates>
<gate name="C" symbol="DISCRETE_CAPACITOR"/>
</gates>
<devices>
<device name="-1210" package="DISCRETE_1210">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2512" package="DISCRETE_2512L">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-A" package="DISCRETE_AVX-A">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-B" package="DISCRETE_AVX-B">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-C" package="DISCRETE_AVX-C">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-D" package="DISCRETE_AVX-D">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-E" package="DISCRETE_AVX-E">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-V" package="DISCRETE_AVX-V">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D5.3/2.0" package="DISCRETE_ELECTRO-5.3MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D8.6/3.81" package="DISCRETE_ELECTRO-8.6MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D11.36/5.08" package="DISCRETE_ELECTRO-11.36MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D20.5/5.1" package="DISCRETE_ELECTROLYTIC-20.5MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-A" package="DISCRETE_ELECTRO-SMD-A-3.8MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-B" package="DISCRETE_ELECTRO-SMD-B-4.8MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-C" package="DISCRETE_ELECTRO-SMD-C-6MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-D" package="DISCRETE_ELECTRO-SMD-D-5.6MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-E" package="DISCRETE_ELECTRO-SMD-E-7.8MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-F" package="DISCRETE_ELECTRO-SMD-F-9.6MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-G" package="DISCRETE_ELECTRO-SMD-G-10MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-UC13/5.08" package="DISCRETE_ELECTRO-13.5MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-UC20/5.08" package="DISCRETE_ELECTRO-20.5MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_CRYSTAL*" prefix="X" uservalue="yes">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
<gates>
<gate name="X" symbol="DISCRETE_Q"/>
</gates>
<devices>
<device name="-3.2X1.5" package="DISCRETE_2P-SMD-3.2X1.5">
<connects>
<connect gate="X" pin="1" pad="P$1"/>
<connect gate="X" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5.08X3.18" package="DISCRETE_2P-SMD-5.08X3.18">
<connects>
<connect gate="X" pin="1" pad="X1"/>
<connect gate="X" pin="2" pad="X2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-6X4" package="DISCRETE_2P-SMD-6X3.6">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-8X5" package="DISCRETE_2P-SMD-8X4.5">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-9.1X3.3" package="DISCRETE_2P-2.0-9.1X3.3">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-9X4.6" package="DISCRETE_2P-2.54-9X4.6">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-86SMX" package="DISCRETE_86SMX">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5032" package="DISCRETE_2P-SMD-5X3.2">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CTS406" package="DISCRETE_CTS406">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC13U-H" package="DISCRETE_HC13U-H">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC18U-H" package="DISCRETE_HC18U-H">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC18U-V" package="DISCRETE_HC18U-V">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC33U-H" package="DISCRETE_HC33U-H">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC33U-V" package="DISCRETE_HC33U-V">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC49GW" package="DISCRETE_HC49GW">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC49S" package="DISCRETE_HC49/S">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC49TL-H" package="DISCRETE_HC49TL-H">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC49U-H" package="DISCRETE_HC49U-H">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC49U-LM" package="DISCRETE_HC49U-LM">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC49U-V" package="DISCRETE_HC49U-V">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC49U70" package="DISCRETE_HC49U70">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC49UP" package="DISCRETE_HC49UP">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MM20SS" package="DISCRETE_MM20SS">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MM39SL" package="DISCRETE_MM39SL">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SM49" package="DISCRETE_SM49">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TC26H" package="DISCRETE_TC26H">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TC26V" package="DISCRETE_TC26V">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TC38H" package="DISCRETE_TC38H">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_D*" prefix="D" uservalue="yes">
<gates>
<gate name="D" symbol="DISCRETE_DIODE"/>
</gates>
<devices>
<device name="3.6" package="DISCRETE_DO-41-3.6">
<connects>
<connect gate="D" pin="+" pad="1"/>
<connect gate="D" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="DISCRETE_SOD123">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SB120" package="DISCRETE_DO-41">
<connects>
<connect gate="D" pin="+" pad="1"/>
<connect gate="D" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1N4148" package="DISCRETE_DO-35">
<connects>
<connect gate="D" pin="+" pad="A"/>
<connect gate="D" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="DISCRETE_SOD523">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0805" package="DISCRETE_SOD323">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1005" package="DISCRETE_D1005">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-B130L-13-F" package="DISCRETE_SMA">
<connects>
<connect gate="D" pin="+" pad="2"/>
<connect gate="D" pin="-" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DO-214AB" package="DISCRETE_DO-214AB">
<connects>
<connect gate="D" pin="+" pad="1"/>
<connect gate="D" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DO-220AA" package="DISCRETE_DO-220AA">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MBR0520LT1" package="DISCRETE_SOD123-2.7X1.6">
<connects>
<connect gate="D" pin="+" pad="2"/>
<connect gate="D" pin="-" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MBRS240LT3" package="DISCRETE_SMB">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMA" package="DISCRETE_D2010">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1N4148-SMD" package="DISCRETE_DO-35-SMD">
<connects>
<connect gate="D" pin="+" pad="A"/>
<connect gate="D" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RL201" package="DISCRETE_DO-15">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1N4148" package="DISCRETE_DO-35">
<connects>
<connect gate="D" pin="+" pad="A"/>
<connect gate="D" pin="-" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="DISCRETE_SOD523">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="DISCRETE_SOD323">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1005" package="DISCRETE_D1005">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B130L-13-F" package="DISCRETE_SMA">
<connects>
<connect gate="D" pin="+" pad="2"/>
<connect gate="D" pin="-" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO-214AB" package="DISCRETE_DO-214AB">
<connects>
<connect gate="D" pin="+" pad="1"/>
<connect gate="D" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO-214AC" package="DISCRETE_D2010">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DO-220AA" package="DISCRETE_DO-220AA">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MBR0520LT1" package="DISCRETE_SOD123-2.7X1.6">
<connects>
<connect gate="D" pin="+" pad="1"/>
<connect gate="D" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MBRS240LT3" package="DISCRETE_SMB">
<connects>
<connect gate="D" pin="+" pad="+"/>
<connect gate="D" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMA" package="DISCRETE_DO-214AC">
<connects>
<connect gate="D" pin="+" pad="1"/>
<connect gate="D" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_LED*" prefix="D" uservalue="yes">
<gates>
<gate name="LED" symbol="DISCRETE_LED"/>
</gates>
<devices>
<device name="0603" package="DISCRETE_LED-0603">
<connects>
<connect gate="LED" pin="+" pad="+"/>
<connect gate="LED" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="DISCRETE_LED-0805">
<connects>
<connect gate="LED" pin="+" pad="+"/>
<connect gate="LED" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TEST" package="DISCRETE_LED-2P-2.54-5MM">
<connects>
<connect gate="LED" pin="+" pad="+"/>
<connect gate="LED" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3MM" package="DISCRETE_LED-2P-2.54-3MM">
<connects>
<connect gate="LED" pin="+" pad="A"/>
<connect gate="LED" pin="-" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-6MM" package="DISCRETE_LED-2P-2.54-6MM">
<connects>
<connect gate="LED" pin="+" pad="+"/>
<connect gate="LED" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-45" package="DISCRETE_LED-2P-2.54-6MM-45D">
<connects>
<connect gate="LED" pin="+" pad="+"/>
<connect gate="LED" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FLSH_LED" package="DISCRETE_LED-2P-2.54-8.5X5-90D">
<connects>
<connect gate="LED" pin="+" pad="+"/>
<connect gate="LED" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SQUARE" package="DISCRETE_LED-2P-2.54-4.8X2.54">
<connects>
<connect gate="LED" pin="+" pad="A"/>
<connect gate="LED" pin="-" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="8MM" package="DISCRETE_2P-SMD-D8.0MM">
<connects>
<connect gate="LED" pin="+" pad="+"/>
<connect gate="LED" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="DISCRETE_LED-0402">
<connects>
<connect gate="LED" pin="+" pad="+"/>
<connect gate="LED" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206" package="DISCRETE_LED-1206">
<connects>
<connect gate="LED" pin="+" pad="+"/>
<connect gate="LED" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3528" package="DISCRETE_LED-3528">
<connects>
<connect gate="LED" pin="+" pad="1"/>
<connect gate="LED" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LEFT" package="DISCRETE_LED-SIDE-VIEW-0603-LEFT">
<connects>
<connect gate="LED" pin="+" pad="1"/>
<connect gate="LED" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RIGHT" package="DISCRETE_LED-SIDE-VIEW-0603-RIGHT">
<connects>
<connect gate="LED" pin="+" pad="1"/>
<connect gate="LED" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_PAD-JUMPER-2P" prefix="P" uservalue="yes">
<gates>
<gate name="G$1" symbol="DISCRETE_JP_SW-1"/>
</gates>
<devices>
<device name="" package="DISCRETE_2P-SMD-1.78X1.27">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_R*" prefix="R" uservalue="yes">
<gates>
<gate name="R" symbol="DISCRETE_R"/>
</gates>
<devices>
<device name="0824/26-5W" package="DISCRETE_0824/26">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0204/5" package="DISCRETE_0204/5">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0204/7" package="DISCRETE_0204/7">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0204SMD" package="DISCRETE_0204SMD">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0204V" package="DISCRETE_0204V">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0207/2V" package="DISCRETE_0207V">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0207/5V" package="DISCRETE_0207/5">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0207/7" package="DISCRETE_0207/7">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0207/10" package="DISCRETE_0207/10">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0207/12" package="DISCRETE_0207/12">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0207SMD" package="DISCRETE_0207SMD">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0309/10" package="DISCRETE_0309/10">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0309/12" package="DISCRETE_0309/12">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0309/15" package="DISCRETE_0309/15">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0309/20" package="DISCRETE_0309/20">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0309V" package="DISCRETE_0309V">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="DISCRETE_0402">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0515''" package="DISCRETE_0515/20.4">
<connects>
<connect gate="R" pin="1" pad="P$1"/>
<connect gate="R" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="DISCRETE_0603">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0805" package="DISCRETE_0805">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0821/27-5W" package="DISCRETE_0821/27">
<connects>
<connect gate="R" pin="1" pad="P$1"/>
<connect gate="R" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1206" package="DISCRETE_1206">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2512" package="DISCRETE_2512">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7519" package="DISCRETE_7519-60.4MM">
<connects>
<connect gate="R" pin="1" pad="1 2"/>
<connect gate="R" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402S" package="DISCRETE_R0402S">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0515" package="DISCRETE_R0515/20.4">
<connects>
<connect gate="R" pin="1" pad="P$1"/>
<connect gate="R" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0824/26-5W" package="DISCRETE_R0824/26">
<connects>
<connect gate="R" pin="1" pad="1 2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE-NEW_CAP" prefix="C" uservalue="yes">
<description>&lt;b&gt;Ceramic Capacitors&lt;b&gt;</description>
<gates>
<gate name="C" symbol="DISCRETE-NEW_C"/>
</gates>
<devices>
<device name="2.54" package="DISCRETE-NEW_PC-D2.286XL5.08MM">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0201" package="DISCRETE-NEW_C0201">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="DISCRETE-NEW_C0402">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="DISCRETE-NEW_C0603">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0805" package="DISCRETE-NEW_C0805">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1206" package="DISCRETE-NEW_C1206">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1210" package="DISCRETE-NEW_C1210">
<connects>
<connect gate="C" pin="1" pad="1"/>
<connect gate="C" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE-NEW_CAP-POLAR" prefix="C" uservalue="yes">
<description>&lt;b&gt;Electrolytic Capacitors,Tantalum Capacitors and Super Capacitors&lt;/b&gt;</description>
<gates>
<gate name="C" symbol="DISCRETE-NEW_CAP-POLAR"/>
</gates>
<devices>
<device name="-AVX-A" package="DISCRETE-NEW_AVX-A">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-B" package="DISCRETE-NEW_AVX-B">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-C" package="DISCRETE-NEW_AVX-C">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-D" package="DISCRETE-NEW_AVX-D">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-E" package="DISCRETE-NEW_AVX-E">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-AVX-V" package="DISCRETE-NEW_AVX-V">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D5.3/2.0" package="DISCRETE-NEW_PC-D5.3MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D8.2/3.05" package="DISCRETE-NEW_PC-D8.2MM">
<connects>
<connect gate="C" pin="+" pad="1"/>
<connect gate="C" pin="-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D8.6/3.81" package="DISCRETE-NEW_PC-D8.6MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D11.36/5.08" package="DISCRETE-NEW_PC-D11.36MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-D20.5/5.1" package="DISCRETE-NEW_PC-D20.5MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-A" package="DISCRETE-NEW_ELECTRO-SMD-A-3.8MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-B" package="DISCRETE-NEW_ELECTRO-SMD-B-4.8MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-C" package="DISCRETE-NEW_ELECTRO-SMD-C-6MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-D" package="DISCRETE-NEW_ELECTRO-SMD-D-5.6MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-E" package="DISCRETE-NEW_ELECTRO-SMD-E-7.8MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-F" package="DISCRETE-NEW_ELECTRO-SMD-F-9.6MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-ELECTRO-G" package="DISCRETE-NEW_ELECTRO-SMD-G-10MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-UC13/5.08" package="DISCRETE-NEW_PC-D13.5MM">
<connects>
<connect gate="C" pin="+" pad="+"/>
<connect gate="C" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE-NEW_CRYSTAL-2P" prefix="X" uservalue="yes">
<gates>
<gate name="X" symbol="DISCRETE-NEW_CRYSTAL"/>
</gates>
<devices>
<device name="3225" package="DISCRETE-NEW_X4-SMD-3.2X2.5X0.7MM">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5032" package="DISCRETE-NEW_X2-SMD-5.0X3.2X1.3MM">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6914" package="DISCRETE-NEW_X4-SMD-6.9X1.4X1.3MM">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="9133" package="DISCRETE-NEW_X2-2.0-D9.1XL3.3MM">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49UP" package="DISCRETE-NEW_HC49UP">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HC49US" package="DISCRETE-NEW_HC49US">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NX2012SA" package="DISCRETE-NEW_X2-SMD-L2.0X1.2X0.55MM">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NX2520SA" package="DISCRETE-NEW_X2-SMD-2.5X2.0X0.5MM">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-3215" package="DISCRETE-NEW_X2-SMD-3.2X1.5X0.55MM">
<connects>
<connect gate="X" pin="1" pad="1"/>
<connect gate="X" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE-NEW_DIODE-BAT54C" prefix="U" uservalue="yes">
<description>Schottky barrier diodes</description>
<gates>
<gate name="G$1" symbol="DISCRETE-NEW_DIODE-BAT54C"/>
</gates>
<devices>
<device name="" package="DISCRETE-NEW_SOT-23">
<connects>
<connect gate="G$1" pin="P$1" pad="1"/>
<connect gate="G$1" pin="P$2" pad="2"/>
<connect gate="G$1" pin="P$3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE-NEW_INDUCTOR/FERRITE-BEAD" prefix="L" uservalue="yes">
<gates>
<gate name="L" symbol="DISCRETE-NEW_L"/>
</gates>
<devices>
<device name="" package="DISCRETE-NEW_INT2-SMD-4.8X4.8X3MM">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6X8H" package="DISCRETE-NEW_INT2-3.5-D6.5XH8.0MM">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="DISCRETE-NEW_L0402">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="DISCRETE-NEW_L0603">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0630" package="DISCRETE-NEW_L0630">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="DISCRETE-NEW_L0805">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0806" package="DISCRETE-NEW_L0806">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1616BZ" package="DISCRETE-NEW_L1616">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1813" package="DISCRETE-NEW_L1813">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2020BZ" package="DISCRETE-NEW_L2020">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2218" package="DISCRETE-NEW_L2218">
<connects>
<connect gate="L" pin="1" pad="P$1"/>
<connect gate="L" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5020" package="DISCRETE-NEW_L5020">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IHLP-2525BD-01" package="DISCRETE-NEW_L2626">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PIO73" package="DISCRETE-NEW_PIO73">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PIO105" package="DISCRETE-NEW_PIO105">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0201" package="DISCRETE-NEW_L0201">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SPD3D16-4R7M" package="DISCRETE-NEW_L0420">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-VLF5010ST-2R2M2R0" package="DISCRETE-NEW_INT2-SMD-4.8X4.6X1.0MM">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5040S" package="DISCRETE-NEW_L5040S">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE-NEW_RES" prefix="R" uservalue="yes">
<gates>
<gate name="R" symbol="DISCRETE-NEW_RES-ARRAY"/>
</gates>
<devices>
<device name="-0201" package="DISCRETE-NEW_R0201">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0204/5" package="DISCRETE-NEW_R0204_5">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0204/7" package="DISCRETE-NEW_R0204_7">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0207/7" package="DISCRETE-NEW_R0207_7">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0207/10" package="DISCRETE-NEW_R0207_10">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0207/12" package="DISCRETE-NEW_R0207_12">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0309/10" package="DISCRETE-NEW_R0309_10">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0309/12" package="DISCRETE-NEW_R0309_12">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0309/15" package="DISCRETE-NEW_R0309_15">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0309/20" package="DISCRETE-NEW_R0309_20">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0402" package="DISCRETE-NEW_R0402">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0515" package="DISCRETE-NEW_R0515_20.4">
<connects>
<connect gate="R" pin="1" pad="P$1"/>
<connect gate="R" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0603" package="DISCRETE-NEW_R0603">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0805" package="DISCRETE-NEW_R0805">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0821/27-5W" package="DISCRETE-NEW_R0821_27">
<connects>
<connect gate="R" pin="1" pad="P$1"/>
<connect gate="R" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0824/26-5W" package="DISCRETE-NEW_R0824_26">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1206" package="DISCRETE-NEW_R1206">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-2512" package="DISCRETE-NEW_R2512">
<connects>
<connect gate="R" pin="1" pad="1"/>
<connect gate="R" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-7519" package="DISCRETE-NEW_R7519_60.4">
<connects>
<connect gate="R" pin="1" pad="1 2"/>
<connect gate="R" pin="2" pad="3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE-NEW_TEST-POINT" prefix="TP" uservalue="yes">
<gates>
<gate name="TP" symbol="DISCRETE-NEW_TEST-POINT"/>
</gates>
<devices>
<device name="" package="DISCRETE-NEW_TP-D65/35MIL">
<connects>
<connect gate="TP" pin="T" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4080" package="DISCRETE-NEW_TP-80X40MIL">
<connects>
<connect gate="TP" pin="T" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4545" package="DISCRETE-NEW_TP-D45MIL">
<connects>
<connect gate="TP" pin="T" pad="T"/>
</connects>
<technologies>
<technology name="">
<attribute name="PARTNO" value="DNP"/>
</technology>
</technologies>
</device>
<device name="-23" package="DISCRETE-NEW_TP-D23MIL">
<connects>
<connect gate="TP" pin="T" pad="T"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-86" package="DISCRETE-NEW_TP-D86MIL">
<connects>
<connect gate="TP" pin="T" pad="T"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-100" package="DISCRETE-NEW_TP-D100MIL">
<connects>
<connect gate="TP" pin="T" pad="T"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FOR_TEST_ALBERT_DC-044" prefix="J">
<gates>
<gate name="JACK" symbol="FOR_TEST_ALBERT_DC-404"/>
</gates>
<devices>
<device name="" package="FOR_TEST_ALBERT_DC-404">
<connects>
<connect gate="JACK" pin="+" pad="+"/>
<connect gate="JACK" pin="-" pad="-"/>
<connect gate="JACK" pin="CDN" pad="CDN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MCP2515" prefix="U">
<description>Stand-Alone CAN Controller With SPI Interface</description>
<gates>
<gate name="G$1" symbol="IC_MCP2515"/>
</gates>
<devices>
<device name="-SOIC18" package="IC_SOIC18">
<connects>
<connect gate="G$1" pin="!CS" pad="16"/>
<connect gate="G$1" pin="!INT" pad="12"/>
<connect gate="G$1" pin="!RESET" pad="17"/>
<connect gate="G$1" pin="!RX0BF" pad="11"/>
<connect gate="G$1" pin="!RX1BF" pad="10"/>
<connect gate="G$1" pin="!TX0RTS" pad="4"/>
<connect gate="G$1" pin="!TX1RTS" pad="5"/>
<connect gate="G$1" pin="!TX2RTS" pad="6"/>
<connect gate="G$1" pin="CLKOUT/SOF" pad="3"/>
<connect gate="G$1" pin="OSC1" pad="8"/>
<connect gate="G$1" pin="OSC2" pad="7"/>
<connect gate="G$1" pin="RXCAN" pad="2"/>
<connect gate="G$1" pin="SCK" pad="13"/>
<connect gate="G$1" pin="SI" pad="14"/>
<connect gate="G$1" pin="SO" pad="15"/>
<connect gate="G$1" pin="TXCAN" pad="1"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC_MCP2551" prefix="U">
<description>High-Speed CAN Transceiver&lt;p/&gt;
http://ww1.microchip.com/downloads/en/devicedoc/21667f.pdf</description>
<gates>
<gate name="G$1" symbol="IC_MCP2551"/>
</gates>
<devices>
<device name="-SOIC8" package="IC_SOIC8-6.0">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC-NEW_AMPLIFIER-MAX2659" prefix="U" uservalue="yes">
<description>GPS/GNSS Low-Noise Amplifier</description>
<gates>
<gate name="G$1" symbol="IC-NEW_AMPLIFIER-MAX2659"/>
</gates>
<devices>
<device name="" package="IC-NEW_DFN6-0.5-1.5X1.2X0.72MM">
<connects>
<connect gate="G$1" pin="!SHDN" pad="5"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="RFIN" pad="3"/>
<connect gate="G$1" pin="RFOUT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="MAX2659"/>
<attribute name="VALUE" value="MAX2659-DFN6"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC-NEW_PMIC-CJ*1117" prefix="U" uservalue="yes">
<description>Low Drop Fixed And Adjustable Positive Voltage Regulators
http://www.datasheetcatalog.org/datasheet/SGSThomsonMicroelectronics/mXuqtqv.pdf</description>
<gates>
<gate name="G$1" symbol="IC-NEW_PMIC-CJ*1117"/>
</gates>
<devices>
<device name="SOT89" package="IC-NEW_SOT-89">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DT" package="IC-NEW_TO-252">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="IC-NEW_SOT-223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2 TER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V" package="IC-NEW_TO-220">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2 HEAT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IC-NEW_RTC-PCF85063TP" prefix="U" uservalue="yes">
<gates>
<gate name="G$1" symbol="IC-NEW_RTC-PCF85063TP"/>
</gates>
<devices>
<device name="" package="IC-NEW_HWSON8-0.5-2X3X0.75MM">
<connects>
<connect gate="G$1" pin="!INT" pad="3"/>
<connect gate="G$1" pin="CLKOUT" pad="7"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="PAD" pad="9"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="POWER-OR-GND-_GND_POWER">
<gates>
<gate name="G$1" symbol="POWER-OR-GND-_GND_POWER"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CAPACITOR_CERAMIC-10UF-25V-10%-X5R(0805)" prefix="C" uservalue="yes">
<description>302010178</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_C"/>
</gates>
<devices>
<device name="" package="SEEED-CAPACITOR_C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0805KKX5R8BB106"/>
<attribute name="VALUE" value="10uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CAPACITOR_CERAMIC-33NF-50V-10%-X7R(0603)" prefix="C" uservalue="yes">
<description>302010088</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_C"/>
</gates>
<devices>
<device name="" package="SEEED-CAPACITOR_C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0603KRX7R9BB333"/>
<attribute name="VALUE" value="33nf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CAPACITOR_CERAMIC-100NF-50V-10%-X7R(0805)" prefix="C" uservalue="yes">
<description>302010165</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_C"/>
</gates>
<devices>
<device name="" package="SEEED-CAPACITOR_C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
<attribute name="VALUE" value="100nf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CAPACITOR_CERAMIC-100PF-50V-5%-NPO(0603)" prefix="C" uservalue="yes">
<description>302010076</description>
<gates>
<gate name="G$1" symbol="SEEED-CAPACITOR_C"/>
</gates>
<devices>
<device name="" package="SEEED-CAPACITOR_C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0603JRNPO9BN101"/>
<attribute name="VALUE" value="100pf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-CONNECTOR_DIP-BLACK-FEMALE-HEADER-VERT(6P-2.54)" prefix="CN">
<description>320030060</description>
<gates>
<gate name="G$1" symbol="SEEED-CONNECTOR_HEADER-6P"/>
</gates>
<devices>
<device name="" package="SEEED-CONNECTOR_H6-2.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="F185-1106A1BSYC1"/>
<attribute name="VALUE" value="6p-2.54"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-IC_LOGIC-TXB0108PW(TSSOP20)" prefix="U" uservalue="yes">
<description>310050024</description>
<gates>
<gate name="G$1" symbol="SEEED-IC_TRANSLATOR-TXS0108E"/>
</gates>
<devices>
<device name="" package="SEEED-IC_TSSOP20-0.65-6.5X4.4MM">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="B1" pad="20"/>
<connect gate="G$1" pin="B2" pad="18"/>
<connect gate="G$1" pin="B3" pad="17"/>
<connect gate="G$1" pin="B4" pad="16"/>
<connect gate="G$1" pin="B5" pad="15"/>
<connect gate="G$1" pin="B6" pad="14"/>
<connect gate="G$1" pin="B7" pad="13"/>
<connect gate="G$1" pin="B8" pad="12"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="OE" pad="10"/>
<connect gate="G$1" pin="VCCA" pad="2"/>
<connect gate="G$1" pin="VCCB" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="TXB0108PW"/>
<attribute name="VALUE" value="TXB0108PW-TSSOP20"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-INDUCTOR_SMD-INDUCTOR-4.7NH-0.3NH-300MA(0402)" prefix="L" uservalue="yes">
<description>303010037</description>
<gates>
<gate name="L" symbol="SEEED-INDUCTOR_SMD-INDUCTOR-4.7NH-0.3NH-300MA(0402)"/>
</gates>
<devices>
<device name="" package="SEEED-INDUCTOR_L0402">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LQG15HS4N7S02"/>
<attribute name="VALUE" value="4.7NH-300MA"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-RESISTOR_SMD-RES-0R-5%-1/10W(0603)" prefix="R" uservalue="yes">
<description>301010292</description>
<gates>
<gate name="G$1" symbol="SEEED-RESISTOR_RES"/>
</gates>
<devices>
<device name="" package="SEEED-RESISTOR_R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0603JR-070RL"/>
<attribute name="VALUE" value="0R"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-RESISTOR_SMD-RES-10K-1%-1/8W(0805)">
<description>301010361</description>
<gates>
<gate name="G$1" symbol="SEEED-RESISTOR_RES"/>
</gates>
<devices>
<device name="" package="SEEED-RESISTOR_R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0805FR-0710KL"/>
<attribute name="VALUE" value="10K"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SEEED-RESISTOR_SMD-RES-100R-5%-1/8W(0805)" prefix="R" uservalue="yes">
<description>301010319</description>
<gates>
<gate name="G$1" symbol="SEEED-RESISTOR_RES"/>
</gates>
<devices>
<device name="" package="SEEED-RESISTOR_R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0805JR-07100RL"/>
<attribute name="VALUE" value="100R"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_L*" prefix="L" uservalue="yes">
<gates>
<gate name="L" symbol="DISCRETE_L"/>
</gates>
<devices>
<device name="-0603S" package="DISCRETE_L0603S">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6X8H" package="DISCRETE_2P-6*8H">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="11.4MM" package="DISCRETE_2P-ROUND-11.4MM">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402" package="DISCRETE_L0402">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0420" package="DISCRETE_L0420">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603" package="DISCRETE_L0603">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0630" package="DISCRETE_L0630">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805" package="DISCRETE_L0805">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0806" package="DISCRETE_0806">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1616BZ" package="DISCRETE_1616BZ">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1813" package="DISCRETE_1813">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2020BZ" package="DISCRETE_2020BZ">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2218" package="DISCRETE_2218">
<connects>
<connect gate="L" pin="1" pad="P$1"/>
<connect gate="L" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5020" package="DISCRETE_5020">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IHLP-2525BD-01" package="DISCRETE_2626">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PIO73" package="DISCRETE_PIO73">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PIO105" package="DISCRETE_PIO105">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-'0402S'" package="DISCRETE_L0402S">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_PAD-TEST-POINT" prefix="TP" uservalue="yes">
<gates>
<gate name="TP" symbol="DISCRETE_TEST_POINT"/>
</gates>
<devices>
<device name="" package="DISCRETE_1P-D6MM">
<connects>
<connect gate="TP" pin="T" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3535" package="DISCRETE_TP_3535">
<connects>
<connect gate="TP" pin="T" pad="T"/>
</connects>
<technologies>
<technology name="">
<attribute name="PARTNO" value="DNP"/>
</technology>
</technologies>
</device>
<device name="4080" package="DISCRETE_PAD_4080">
<connects>
<connect gate="TP" pin="T" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4545" package="DISCRETE_TP_4545">
<connects>
<connect gate="TP" pin="T" pad="T"/>
</connects>
<technologies>
<technology name="">
<attribute name="PARTNO" value="DNP"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_RELAY-HLS8L-DC5V-S-C" prefix="SW" uservalue="yes">
<gates>
<gate name="G$1" symbol="DISCRETE_RELAY"/>
</gates>
<devices>
<device name="" package="DISCRETE_5P-19.0X15.5X15.8H">
<connects>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="NO" pad="4"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DISCRETE_TRANSISTOR-NPN*" prefix="Q" uservalue="yes">
<description>&lt;b&gt;NPN audion&lt;b&gt;&lt;p&gt;</description>
<gates>
<gate name="Q" symbol="DISCRETE_NPN"/>
</gates>
<devices>
<device name="-1.27" package="DISCRETE_NPN1.27">
<connects>
<connect gate="Q" pin="B" pad="B"/>
<connect gate="Q" pin="C" pad="C"/>
<connect gate="Q" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOT23" package="DISCRETE_SOT23">
<connects>
<connect gate="Q" pin="B" pad="1"/>
<connect gate="Q" pin="C" pad="3"/>
<connect gate="Q" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOT323" package="DISCRETE_SOT323">
<connects>
<connect gate="Q" pin="B" pad="1"/>
<connect gate="Q" pin="C" pad="3"/>
<connect gate="Q" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO-92" package="DISCRETE_TO-92-TRIANGLE">
<connects>
<connect gate="Q" pin="B" pad="1"/>
<connect gate="Q" pin="C" pad="3"/>
<connect gate="Q" pin="E" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOUDLE-NEW_MOUDLE-GPS-L70-HARDWARE" prefix="U" uservalue="yes">
<description>L70 GPS module</description>
<gates>
<gate name="G$1" symbol="MOUDLE-NEW_MOUDLE-GPS-L70-HARDWARE"/>
</gates>
<devices>
<device name="" package="MOUDLE-NEW_LGA18-1.1-9.7X10.1X2.5MM">
<connects>
<connect gate="G$1" pin="1PPS" pad="4"/>
<connect gate="G$1" pin="ANTON" pad="13"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC@1" pad="15"/>
<connect gate="G$1" pin="RESERVED" pad="16"/>
<connect gate="G$1" pin="RESERVED1" pad="17"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="RF_IN" pad="11"/>
<connect gate="G$1" pin="RXD1" pad="3"/>
<connect gate="G$1" pin="STANDBY" pad="5"/>
<connect gate="G$1" pin="TIMER" pad="18"/>
<connect gate="G$1" pin="TXD1" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VCC_RF" pad="14"/>
<connect gate="G$1" pin="V_BCKP" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="L70"/>
<attribute name="VALUE" value="L70"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RASPBERRYPI_BASTELSTUBE_V13_RASPI_GPIO_AB" prefix="X">
<description>Only the 2x13 header connector, nothing else</description>
<gates>
<gate name="G$1" symbol="RASPBERRYPI_BASTELSTUBE_V13_RASPI_GPIO_AB"/>
</gates>
<devices>
<device name="_BOX" package="RASPBERRYPI_BASTELSTUBE_V13_RASPI_GPIO_AB_BOX">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_PIN" package="RASPBERRYPI_BASTELSTUBE_V13_RASPI_GPIO_AB_PIN">
<connects>
<connect gate="G$1" pin="3V3" pad="1"/>
<connect gate="G$1" pin="5V0" pad="2"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GPIO04" pad="7"/>
<connect gate="G$1" pin="GPIO17" pad="11"/>
<connect gate="G$1" pin="GPIO18" pad="12"/>
<connect gate="G$1" pin="GPIO22" pad="15"/>
<connect gate="G$1" pin="GPIO23" pad="16"/>
<connect gate="G$1" pin="GPIO24" pad="18"/>
<connect gate="G$1" pin="GPIO25" pad="22"/>
<connect gate="G$1" pin="GPIO27" pad="13"/>
<connect gate="G$1" pin="N.C.0" pad="4"/>
<connect gate="G$1" pin="N.C.1" pad="9"/>
<connect gate="G$1" pin="N.C.2" pad="14"/>
<connect gate="G$1" pin="N.C.3" pad="17"/>
<connect gate="G$1" pin="N.C.4" pad="20"/>
<connect gate="G$1" pin="N.C.5" pad="25"/>
<connect gate="G$1" pin="RXD" pad="10"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="3"/>
<connect gate="G$1" pin="SPI_CE0" pad="24"/>
<connect gate="G$1" pin="SPI_CE1" pad="26"/>
<connect gate="G$1" pin="SPI_MISO" pad="21"/>
<connect gate="G$1" pin="SPI_MOSI" pad="19"/>
<connect gate="G$1" pin="SPI_SCLK" pad="23"/>
<connect gate="G$1" pin="TXD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEMPLATE_MP1496DJ" prefix="U" uservalue="yes">
<description>High-Efficiency,2A，16V,500kHz Synchronous,Step-Down Converter&lt;p/&gt;
http://html.alldatasheetcn.com/html-pdf/551584/MPS/MP1496DJ/55/1/MP1496DJ.html</description>
<gates>
<gate name="G$1" symbol="TEMPLATE_MP1496"/>
</gates>
<devices>
<device name="" package="TEMPLATE_TSOT23-8">
<connects>
<connect gate="G$1" pin="BS" pad="5"/>
<connect gate="G$1" pin="EN/SYNC" pad="6"/>
<connect gate="G$1" pin="FB" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="SS" pad="1"/>
<connect gate="G$1" pin="SW" pad="3"/>
<connect gate="G$1" pin="VCC" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
